*****************This FW only for X722 PHY board NVM Online-Auto update Tool program*******************
================================================================================================
3GS5BMA0090 / ON 10GbE X722-X557-T4 RJ45 MEZZ Online-Auto update NVM Release Note 
3GS5BMA00C0 / ON 10GbE X722-X557-T2 RJ45 MEZZ Online-Auto update NVM Release Note
3GS5BMA00I0 / ON 10GbE X722-X557-T4 RJ45 HS2 MEZZ Online-Auto update NVM Release Note
3GS5BMA00E0 / ON 10GbE X722-X527-DA2 SFP plus MEZZ Online-Auto update NVM Release Note
3GS5BMA00A0 / ON 10GbE X722-X527-DA4 SFP plus MEZZ Online-Auto update NVM Release Note
3GS5BMA00D0 / ON 1GbE X722-I357-T2 RJ45  MEZZ Online-Auto update NVM Release Note
3GS5BMA00B0 / ON 1GbE X722-I357-T4 RJ45  MEZZ Online-Auto update NVM Release Note
================================================================================================
Quanta FW file package: 2018_WW46_LBG_X722_NUP_UEFI_0006
Release day: 2018/12/20

Change history
12/20
1.Fix Malicious Driver Detection (MDD) Event issue will cause Network Dropout/ignition miss
( The MDD is fixed in 1.7.11 and the firmware required for this driver is 4.00)
04/22
1.NVM 0005 Fix Port lost issue
================================================================================================
NVMUPDATE Tool version:1.32.20.29


================================================================================================
================================================================================================

Update procedure:

[UEFI version]
1.Excute the tool "nvmupdate64e.efi"under UEFI mode
2.Option:Adapter Index List(comma-separated),[A]ll, e[X]it Enter selection:A
3.Would you like to back up the NVM images?[Y]es/[N]o: N
4.Waiting for the tool updating, and do not power off the system
5.After the tool update complete, please must restart the system.

[Check the version after reboot the system]
1.Excute the tool "./nvmupdate64e -i -l"
2.Check the NVM version item, it should be 4.00

end of the procedure