;/*++
;
;Copyright (c) 2001-2004 Atheros Communications, Incorporated All Rights Reserved
;
;Module Name:
;
;    net5211.inf
;
;Abstract:
;    INF file for installing Atheros Wireless Network Adapter Family
;
;    Installs ar5211.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs ar52119x.sys (NDIS 5 driver) on 9x platforms 
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
Compatible  = 1
DriverVer   = 07/22/2004,3.1.102.23

Catalogfile = net5211.cat

[Manufacturer]
%ATHEROS%     = Atheros,NTx86.5.1

[ControlFlags]
ExcludeFromSelect = *

[Atheros]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic

; Bartlett
%ATHER.DeviceDesc.0014%  = ATHER_DEV_2013,    PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
; Clymer
%ATHER.DeviceDesc.1013%  = ATHER_DEV_1013,    PCI\VEN_168C&DEV_0013&SUBSYS_04081468
; Radon
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013,    PCI\VEN_168C&DEV_1014&SUBSYS_833117ab
; Argon
%ATHER.DeviceDesc.2022%  = ATHER_DEV_2022,    PCI\VEN_168C&DEV_0012&SUBSYS_831017ab

[Atheros.NTx86.5.1]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic

; Bartlett
%ATHER.DeviceDesc.0014%  = XP_DEV_2013,    PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
; Clymer
%ATHER.DeviceDesc.1013%  = XP_DEV_1013,    PCI\VEN_168C&DEV_0013&SUBSYS_04081468
; Radon
%ATHER.DeviceDesc.0013%  = XP_DEV_0013,    PCI\VEN_168C&DEV_1014&SUBSYS_833117ab
; Argon
%ATHER.DeviceDesc.2022%  = XP_DEV_2022,    PCI\VEN_168C&DEV_0012&SUBSYS_831017ab

; Windows 9X specific entries

[ATHER_DEV_2022]
DelReg          = 5211.DelReg
AddReg          = ATHER_DEV_2022.id.reg, 5211.reg, ATHER.win.reg, 5211.abmp.reg
CopyFiles       = ATHER.win.CopyFiles 
DelFiles        = ATHER.DelIniFiles


[ATHER_DEV_0013]
DelReg          = 5211.DelReg
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212.abg.reg
CopyFiles       = ATHER.win.CopyFiles
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1013]
DelReg          = 5211.DelReg
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
CopyFiles       = ATHER.win.CopyFiles
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2013]
DelReg          = 5211.DelReg
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5213.abg.reg
CopyFiles       = ATHER.win.CopyFiles
DelFiles        = ATHER.DelIniFiles

; Windows NT specific entries

[ATHER_DEV_2022.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS1.reg, 5211.abmp.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles


[ATHER_DEV_0013.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS1.reg, 5212.abg.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1013.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS1.reg, 5212.bgmp.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2013.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS1.reg, 5213.abg.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2022.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0013.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1013.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog


[ATHER_DEV_2013.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

;;Windows XP specific entries

[XP_DEV_2022]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS2.reg, 5211.abmp.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[XP_DEV_0013]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS2.reg, 5212.abg.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[XP_DEV_1013]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS2.reg, 5212.bgmp.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[XP_DEV_2013]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, PS2.reg, 5213.abg.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[XP_DEV_2022.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[XP_DEV_0013.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[XP_DEV_1013.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog


[XP_DEV_2013.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

;---------------------------------------------------------
;
; 5211 Enumerated Types
;

[5211.abmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "15"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

HKR,NDI\params\TransmitRate11a,ParamDesc,,	"11a Transmit Rates"
HKR,NDI\params\TransmitRate11a,type,,		"enum"
HKR,NDI\params\TransmitRate11a,Default,,	"7"

HKR,NDI\params\TransmitRate11a\enum,0,,		"6 Mbps"
HKR,NDI\params\TransmitRate11a\enum,1,,		"9 Mbps"
HKR,NDI\params\TransmitRate11a\enum,2,,		"12 Mbps"
HKR,NDI\params\TransmitRate11a\enum,3,,		"18 Mbps"
HKR,NDI\params\TransmitRate11a\enum,4,,		"24 Mbps"
HKR,NDI\params\TransmitRate11a\enum,5,,		"36 Mbps"
HKR,NDI\params\TransmitRate11a\enum,6,,		"48 Mbps"
HKR,NDI\params\TransmitRate11a\enum,7,,		"54 Mbps"

;Following Entry made to Enable/Disable Ext Channel Mode through Device Manager.

HKR, Ndi\params\extendedChanMode,          ParamDesc,                      0,  "Extended Channel Mode"
HKR, Ndi\params\extendedChanMode,          Base,                           0,  "10"
HKR, Ndi\params\extendedChanMode,          default,                        0,  "0"
HKR, Ndi\params\extendedChanMode,          type,                           0,  "enum"
HKR, Ndi\params\extendedChanMode\enum,     "1",                            0,  "Enable"
HKR, Ndi\params\extendedChanMode\enum,     "0",                            0,  "Disable(for N,America)"

HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "15"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "15",                           0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "3",                            0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "12",                            0,  "2.4Ghz Only"


[5212.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "15"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

HKR,NDI\params\TransmitRate11g,ParamDesc,,	"11g Transmit Rates"
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11g\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11g\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11g\enum,3,,		"11 Mbps"
HKR,NDI\params\TransmitRate11g\enum,4,,		"6 Mbps"
HKR,NDI\params\TransmitRate11g\enum,5,,		"9 Mbps"
HKR,NDI\params\TransmitRate11g\enum,6,,		"12 Mbps"
HKR,NDI\params\TransmitRate11g\enum,7,,		"18 Mbps"
HKR,NDI\params\TransmitRate11g\enum,8,,		"24 Mbps"
HKR,NDI\params\TransmitRate11g\enum,9,,		"36 Mbps"
HKR,NDI\params\TransmitRate11g\enum,10,,	"48 Mbps"
HKR,NDI\params\TransmitRate11g\enum,11,,	"54 Mbps"

[5212.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "15"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR,NDI\params\TransmitRate11g,ParamDesc,,	"11g Transmit Rates"
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11g\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11g\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11g\enum,3,,		"11 Mbps"
HKR,NDI\params\TransmitRate11g\enum,4,,		"6 Mbps"
HKR,NDI\params\TransmitRate11g\enum,5,,		"9 Mbps"
HKR,NDI\params\TransmitRate11g\enum,6,,		"12 Mbps"
HKR,NDI\params\TransmitRate11g\enum,7,,		"18 Mbps"
HKR,NDI\params\TransmitRate11g\enum,8,,		"24 Mbps"
HKR,NDI\params\TransmitRate11g\enum,9,,		"36 Mbps"
HKR,NDI\params\TransmitRate11g\enum,10,,	"48 Mbps"
HKR,NDI\params\TransmitRate11g\enum,11,,	"54 Mbps"


HKR,NDI\params\TransmitRate11a,ParamDesc,,	"11a Transmit Rates"
HKR,NDI\params\TransmitRate11a,type,,		"enum"
HKR,NDI\params\TransmitRate11a,Default,,	"7"

HKR,NDI\params\TransmitRate11a\enum,0,,		"6 Mbps"
HKR,NDI\params\TransmitRate11a\enum,1,,		"9 Mbps"
HKR,NDI\params\TransmitRate11a\enum,2,,		"12 Mbps"
HKR,NDI\params\TransmitRate11a\enum,3,,		"18 Mbps"
HKR,NDI\params\TransmitRate11a\enum,4,,		"24 Mbps"
HKR,NDI\params\TransmitRate11a\enum,5,,		"36 Mbps"
HKR,NDI\params\TransmitRate11a\enum,6,,		"48 Mbps"
HKR,NDI\params\TransmitRate11a\enum,7,,		"54 Mbps"

;Following Entry made to Enable/Disable Ext Channel Mode through Device Manager.

HKR, Ndi\params\extendedChanMode,          ParamDesc,                      0,  "Extended Channel Mode"
HKR, Ndi\params\extendedChanMode,          Base,                           0,  "10"
HKR, Ndi\params\extendedChanMode,          default,                        0,  "0"
HKR, Ndi\params\extendedChanMode,          type,                           0,  "enum"
HKR, Ndi\params\extendedChanMode\enum,     "1",                            0,  "Enable"
HKR, Ndi\params\extendedChanMode\enum,     "0",                            0,  "Disable(for N,America)"

HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "15"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "15",                           0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "3",                            0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "12",                           0,  "2.4Ghz Only"

[5213.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "15"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR,NDI\params\TransmitRate11g,ParamDesc,,	"11g Transmit Rates"
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11g\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11g\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11g\enum,3,,		"11 Mbps"
HKR,NDI\params\TransmitRate11g\enum,4,,		"6 Mbps"
HKR,NDI\params\TransmitRate11g\enum,5,,		"9 Mbps"
HKR,NDI\params\TransmitRate11g\enum,6,,		"12 Mbps"
HKR,NDI\params\TransmitRate11g\enum,7,,		"18 Mbps"
HKR,NDI\params\TransmitRate11g\enum,8,,		"24 Mbps"
HKR,NDI\params\TransmitRate11g\enum,9,,		"36 Mbps"
HKR,NDI\params\TransmitRate11g\enum,10,,	"48 Mbps"
HKR,NDI\params\TransmitRate11g\enum,11,,	"54 Mbps"


HKR,NDI\params\TransmitRate11a,ParamDesc,,	"11a Transmit Rates"
HKR,NDI\params\TransmitRate11a,type,,		"enum"
HKR,NDI\params\TransmitRate11a,Default,,	"7"

HKR,NDI\params\TransmitRate11a\enum,0,,		"6 Mbps"
HKR,NDI\params\TransmitRate11a\enum,1,,		"9 Mbps"
HKR,NDI\params\TransmitRate11a\enum,2,,		"12 Mbps"
HKR,NDI\params\TransmitRate11a\enum,3,,		"18 Mbps"
HKR,NDI\params\TransmitRate11a\enum,4,,		"24 Mbps"
HKR,NDI\params\TransmitRate11a\enum,5,,		"36 Mbps"
HKR,NDI\params\TransmitRate11a\enum,6,,		"48 Mbps"
HKR,NDI\params\TransmitRate11a\enum,7,,		"54 Mbps"

HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "15"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "15",                           0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "3",                            0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "12",                           0,  "2.4Ghz Only"




;-----------------------------------------------------------------------------

;
; 5211 common
;

[5211.DelReg]
HKR,,NetBand
;HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
;HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin

HKR, Ndi\params\ExtendedChannel
HKR, NDI\params\Mode11dSwitch
HKR, Ndi\params\MapRegisters

HKR, CustomParams\Configurations\Cfg0

[5211.reg]

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          default,                        0,  "45000"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "enum"
HKR, Ndi\params\scanTimeValid\enum,     "120000",                       0,  "120"
HKR, Ndi\params\scanTimeValid\enum,     "60000",                        0,  "60"
HKR, Ndi\params\scanTimeValid\enum,     "45000",                        0,  "45"
HKR, Ndi\params\scanTimeValid\enum,     "30000",                        0,  "30"
HKR, Ndi\params\scanTimeValid\enum,     "20000",                        0,  "20"
HKR, Ndi\params\scanTimeValid\enum,     "10000",                        0,  "10"
HKR, Ndi\params\scanTimeValid\enum,     "5000",                         0,  "5"

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%




;Following Entry made to Enable/Disable rate Auto Rate control.

HKR,NDI\params\rateCtrlEnable,ParamDesc,,	"Auto Transmit Rate"
HKR,NDI\params\rateCtrlEnable,type,,		"enum"
HKR,NDI\params\rateCtrlEnable,Default,,		"1"
HKR,NDI\params\rateCtrlEnable\enum,0,,		"Disable"
HKR,NDI\params\rateCtrlEnable\enum,1,,		"Enable"

;Following Entry made to 11d mode switch 

HKR,NDI\params\ignore11dBeacon,ParamDesc,,	"11d Mode Switch"
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		"Enable"
HKR,NDI\params\ignore11dBeacon\enum,1,,		"Disable"

HKR,NDI\params\TransmitRate11b,ParamDesc,,	"11b Transmit Rates"
HKR,NDI\params\TransmitRate11b,type,,		"enum"
HKR,NDI\params\TransmitRate11b,Default,,	"3"

HKR,NDI\params\TransmitRate11b\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11b\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11b\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11b\enum,3,,		"11 Mbps"

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"
HKR, ,					scanTimePreSleep,               0x00002,  "60" ; New Entry for IBM.

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"


[PS1.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  1 ;Set power Mgmt mode to Max.
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

[PS2.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  2 ;Set power Mgmt mode to Normal.
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

; Allow non admin uses to switch profiles
[5211.reg.security]
"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR5211"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"



[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ar5211.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; ATHER Win9x specific
;
[ATHER.win.reg]
HKR, ,                  DevLoader,          0,    "*ndis"
HKR, ,                  DeviceVxDs,         0,    "ar52119x.sys"
HKR, ,                  EnumPropPages,      0,    "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,    DefUpper,           0,    "ndis3"
HKR, Ndi\Interfaces,    DefLower,           0,    "ethernet"
HKR, Ndi\Interfaces,    UpperRange,         0,    "ndis3"
HKR, Ndi\Interfaces,    LowerRange,         0,    "ethernet"


HKR, NDIS,              LogDriverName,      0,    "AR52119X"
HKR, NDIS,              MajorNdisVersion,   1,    03
HKR, NDIS,              MinorNdisVersion,   1,    0A


HKR, Ndi\Install,       ndis3,              0,    "ATHER.install"

;----------------------------------------------------------------------------
; Win9x Files to Copy
[ATHER.win.CopyFiles]
ar52119x.sys,,,2

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
ar5211.sys,,,2





[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %Atheros_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
ar52119x.sys                 = 1,, ; on distribution disk 1
ar5211.sys                   = 1,, ; on distribution disk 1

[DestinationDirs]
ATHER.CopyFiles.nt           = 12
ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers 
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers 
DefaultDestDir               = 11

[Strings]
Atheros                      = "Atheros Communications Inc"
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
scanTimeValid                = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode         	     = "Wireless Mode Selection"



Atheros_Disk                 = "Driver Disk 1"
 

ATHER.DeviceDesc.1013        = "11b/g Wireless LAN Mini PCI Adapter"
ATHER.DeviceDesc.0014        = "11a/b/g Wireless LAN Mini PCI Adapter II"   
ATHER.DeviceDesc.2022        = "Dual-band Wi-Fi Wireless Mini PCI Adapter"
ATHER.DeviceDesc.0013        = "11a/b/g Wireless LAN Mini PCI Adapter"
ATHER.Service.DispName       = "Dual-band Wi-Fi Wireless Mini PCI Adapter"

