Quick Flash Instructions For AMI Motherboards:
(FLASH UTILITY NOT REQUIRED)


- Unzip file, copy the "ROM" file to a diskette in "A" drive.            
               (Diskette does not have to be bootable).

- Make sure you are using the on board floppy controller.

- With system powered off and diskette with "ROM" file in "A" drive.

- Hold down on the "CTRL & HOME" keys and then power on system.

- There will be no video and notice floppy drive being accessed.

- You should hear 1 beep let go of keys.

- Then you will hear 2 beeps and then 3 beeps.

- System should reset and notice new BIOS release date at top of screen.

- Enter BIOS SETUP run the OPTIMAL SETINGS OPTION.

- Change BIOS SETTINGS for your configuration.


"WARNING"
If you are using the "password" option in the BIOS, you must DISABLE the
Password BEFORE you flashes the BIOS. This BIOS uses a new core and saves the 
Password at a different location.

If you flash the BIOS without disabling the password, you may not be able
To get into the setup. If this happens, you must drain the CMOS first.


**November 9, 2000**