#ident	"@(#)README	1.2	90/03/16 SMI"	/* SVr4.0 1.2	*/
Source code in this directory is for the program that can be used to send files
to printers that understand PostScript.

I've added code that lets you split the program into separate read and write
processes (the -R2 option), supports an interactive mode (-i option), suppresses
status queries while the files are being transmitted to the printer (-q option),
and runs in a mode that can help if flow control doesn't appear to be working
properly (-S option). All the options are described in the man page. In addition
The parsing of lines returned by the printer has been improved and should do a
decent job with anything that comes its way.

By default the program runs much like the original version - a single process with
status queries sent every block or two. It's not how to get the best performance,
but using a single read/write process may be important if you're running lots of
printers under a single userid. Four things can help improve performance, and all
can be set by command line options:

 1: Use separate read and write processes. The -R2 option gets it or if you want
    it as the default initialize splitme (near line 132 in postio.c) to TRUE before
    compiling postio.

 2: Use a large input buffer. The default size is 2048 bytes, but it can be set
    to whatever you want on the command line using the -B option. If you want a
    larger default buffer change the definition of BLOCKSIZE (near line 204 in
    postio.h) before you compile postio.

 3: Quiet mode prevents the transmission of status requests (ie. ^Ts) while files
    are being sent to the printer. You can turn off the status query stuff with
    the -q option or if you want it as the default initialize quiet (near line 122
    in postio.c) to TRUE before compiling the program.

 4: Avoid using the -S option. It's real slow and I thought some about leaving it
    out, but it's needed at a few sites. Seems to help most with printers connected
    to UTS systems using DACUs and Datakit PVCs.

One possible strategy would be to have the spooler run postio as a single process
on all small printers (eg. LaserWriters or PS-800s) and use two processes on faster
printers like the DataProducts 2665 or QMS PS-2400.

A typical command line might look something like,

    postio -l /dev/tty?? -b 9600 -L log file1 file2 file3

where /dev/tty?? is the line that's connected to the printer, 9600 (or B9600) is
the baud rate, and log is a file used to record printer status. You should always
use the -l option to select the printer line, and if you don't choose a log file
everything coming back from the printer goes to stderr. The following command line
accomplishes the same thing, but runs postio as separate read and write processes,

    postio -R2 -l/dev/tty?? -b9600 -Llog file1 file2 file3

Check the man page for more examples.

