AlphaBIOS V5.69
25 May 1999

렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁

This zip file contains V5.68 NT AlphaBIOS Multiboot firmware and installation 
instructions for these systems:

    Compaq AlphaServer DS20
    Compaq AlphaPC 264DP

This new firmware supports:

    Windows NT Workstation Version 4.00
    Windows NT Server Version 4.00

For information on the specific changes in this AlphaBIOS release, please 
consult the AlphaBIOS V5.68 Release Notes.


Updating the Firmware

1.  To install this firmware, unzip this kit into the root directory
    on a blank, formatted floppy disk.

    Label this floppy "V5.69 DS20/264DP firmware."

    Compaq generally recommends that you update both the AlphaBIOS and the SRM 
    firmware to the latest available released versions.  This release includes
    current SRM firmware version.

2.  If running NT, shut down and reboot the system.  This may be done
    by selecting the "Shutdown and Restart" option in the "Shutdown
    Computer" logoff popup window.  Proceed onto the next step when
    you are at the AlphaBIOS Boot Menu.

3.  When the AlphaBIOS Boot Menu appears, note the version at the top of 
    the screen.

    If it is 5.69 or later, then congratulations!  You already have this
    (or a newer) firmware installed and you do not need to update your firmware.
    To install Windows NT, read the Configuration Guide (or Release Notes) 
    that came with your Windows NT kit.  You can also obtain a copy of the 
    Configuration Guide at our World Wide Web site, at 
    http://www.compaq.com/support/files/alphant/index.html
    
    If the current AlphaBIOS version is not 5.69 or above, then an update 
    of the firmware may be needed in order to run Windows NT; proceed to 
    step 4 to upgrade.

4.  Insert the "V5.69 DS20/264DP firmware" floppy into your
    floppy drive.

5.  Press F2 to enter the Setup menu.

6.  Select "Upgrade AlphaBIOS" and press Enter.

7.  The update process begins. 

       a.  The floppy, CDROM, and an optional network server are searched
           (in that order) for the platform AlphaBIOS binary.  Once located, the
           image is read into memory.

       b.  Next, AlphaBIOS will prompt you to confirm the intent to
           upgrade AlphaBIOS to V5.69.  Press F10 to commit and begin the
           upgrade process.
 
       c.  When the upgrade is complete, a dialog box will appear indicating
           the need to press Enter to execute the newly-loaded firmware image.
           Press Enter and the system will reboot.  The AlphaBIOS firmware
           image is now updated and you can remove the floppy.


    If you encounter any difficulties in updating the firmware, call the 
    DIGITAL technical support line for further assistance.  In the U.S.A the
    telephone number is (800)354-9000.


    Your firmware update is complete.

렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁렁
