INF: LIM-EMS Memory Limitations in a Windows NT VDM
PSS ID Number: Q101189
Article last modified on 04-23-1994

3.10

WINDOWS NT


----------------------------------------------------------------------
The information in this article applies to:

 - Microsoft Win32 Software Development Kit (SDK) for Windows NT,
   version 3.1
----------------------------------------------------------------------

A Windows NT virtual MS-DOS machine (VDM) session is LIM-EMS 4.0
compatible; however, each VDM is limited to 16 megabytes (MB) of memory.

A VDM is an MS-DOS session created whenever a user starts an MS-DOS
application on Windows NT. Windows NT allows any number of MS-DOS
applications to run simultaneously, each in its own address space.

Additional reference words: 3.10
KBCategory: Prg
KBSubcategory: SubSys

=============================================================================

Copyright Microsoft Corporation 1994.
