Hardware Compat. List: Other Tape Drives - ISDN Adapters
  
PSS ID Number: Q101576
Article last modified on 03-07-1995
 
3.10
 
WINDOWS
 

----------------------------------------------------------------------
The information in this article applies to:
 
 - Microsoft Windows NT operating system version 3.1
----------------------------------------------------------------------
 
Other Tape Drives
=================
 
The following tape drives have been tested using the Windows NT Backup
utility.
 
QIC-40/QIC-80 Floppy Tape Drive [36]
------------------------------------
 
   Archive 5150Q (SuperHornet)
   Archive 5540
   Archive 5580
   Colorado Memory Systems Jumbo 250
   Iomega Tape 250
   Summit Express SE120
   Summit Express SE250
   WangTek 3040
   WangTek 3080
 
SCSI Removable Media
====================
 
The following removable media (cartridge) drives have been tested with
the following adapters: Adaptec AHA-1510, AHA-1542C, AHA-1640 and AHA-
1742A; Future Domain TMC-1670, TMC-850M and MCS-600; IBM PS/2
Microchannel SCSI Host Adapter (with cache); Ultrastor 24fa.  Media
must be mounted when installing Windows NT.
 
Hewlett-Packard Series 6300 650/C [37]
IBM 0632 Model C2* [34, 37]
Insite 21mb Floptical
Iomega 21mb Floptical
Iomega Bernoulli Transportable 90 Pro
Iomega Bernoulli Transportable 150
Peripheral Land Infinity 40 Turbo
Peripheral Land Infinity 88
Quantum Passport XL 85
Quantum Passport XL 127
Sony SMO-S511A-11 [37]
Sony RMO-S350
Syquest ® 555 44mb cartridge
Syquest 5110 88mb cartridge
 
SCSI Scanners
=============
 
The following scanners have been tested with the following adapters:
Adaptec AHA-1510, AHA-1542c, AHA-1640 and AHA-1742A; Future Domain
TMC-1670, TMC-850M and MCS-600; IBM PS/2 Microchannel SCSI Host
Adapter (with cache); Ultrastor 24fa.
 
HP ScanJet ® IIc
HP ScanJet IIp
 
Disk Controllers
================
 
The following disk controllers have been tested.
 
COMPAQ Intelligent Drive Array Controller
COMPAQ Intelligent Drive Array Controller-2
COMPAQ SMART Array Controller
DELL Drive Array Controller
DELL SCSI Array Controller [1]
Western Digital ® 1003 (ESDI, IDE)
 
Storage Cabinets
================
 
The following peripheral storage cabinets have been tested.
 
Hewlett-Packard Storage System with HP EISA HBA [38]
Hewlett-Packard Storage System with HP MCA HBA [38]
 
Video Display Support
=====================
 
The following display adapters have been tested. Most common scan
frequencies are supported. Your video monitor should support the same
resolutions and scan frequencies as your display adapter. Please refer
to README.WRI for more information on display support.
 
                                640x480   800x600   1024x768
Display Adapter      Driver     x16 x256  x16 x256  x16 x256  Other
---------------      --------   --------  --------  --------  --------
 
ACTIX GRAPHICS       S3              NI        NI        NI
    ENGINE
ACTIX GRAPHICS       S3              NI        NI        NI
    ENGINE 32 PLUS
ATI 8514 ULTRA       ATI             NI        NI        NI
ATI GRAPHICS ULTRA   ATI             NI        NI        NI   2, 3, 4, 5,
    PRO                                                       6, 7, 11
ATI GRAPHICS ULTRA   ATI             NI        NI        NI   2, 3, 4, 5,
    PRO VLB                                                   6, 7, 11
ATI GRAPHICS ULTRA   ATI             NI        NI        NI   2, 3, 4, 5,
    PLUS                                                      6, 7, 11
ATI GRAPHICS ULTRA   ATI             NI        NI        NI
ATI GRAPHICS         ATI             NI        NI        NI
    VANTAGE
COMPAQ AVGA          ++AVGA     NI   NI   NI
COMPAQ QVISION       QVISION         NI        NI        NI
    1024/I
COMPAQ QVISION       QVISION         NI        NI        NI
    1024/E
COMPAQ QVISION       QVISION         NI        NI        NI
    1024/I (ENHANCED)
COMPAQ QVISION       QVISION         NI        NI        NI
    1024/E (ENHANCED)
COMPAQ QVISION       QVISION         NI        NI        NI   11
    1280/I
COMPAQ QVISION       QVISION    NI   NI   NI   NI        NI   11
    1280/E
DELL DGX             DGX             NI        NI        NI   2, 5, 7, 9,
                                                              10, 11
DIAMOND SPEEDSTAR    ET4000     NI   NI   NI   NI    B    B
DIAMOND SPEEDSTAR    WD         NI   NI   NI   NI    B    B
    24X
DIAMOND SPEEDSTAR    CIRRUS     NI   NI   NI   NI   NI   NI
    PRO & PRO VLB
DIAMOND STEALTH 24   S3              NI        NI        NI
DIAMOND STEALTH 24   S3              NI        NI        NI
    VLB
DIAMOND STEALTH PRO  S3              NI        NI        NI
    & PRO VLB
DIAMOND STEALTH      S3              NI        NI        NI
    VRAM
ELSA WINNER 1000     S3              NI        NI        NI
GENOA VLB            CIRRUS     NI   NI   NI   NI   NI   NI
IBM XGA              XGA             NI                   I
IBM XGA-2            XGA             NI        NI         B   1, 8
MEDIAVISION THUNDER  CIRRUS     NI   NI   NI   NI   NI   NI
    & LIGHTNING
METHEUS PREMIER 928  S3              NI        NI        NI
METHEUS PREMIER      S3              NI        NI        NI
    VL-BUS 928
MICRONICS VL-BUS     S3              NI        NI        NI
NCR 77C22            NCR77C22   NI   NI   NI   NI   NI
NCR 77C22E           NCR77C22   NI   NI   NI   NI   NI   NI
NUMBER 9 GXE         S3              NI        NI        NI   11
ORCHID FAHRENHEIT    S3              NI        NI        NI
    1280
ORCHID FAHRENHEIT    S3              NI        NI        NI
    VA
ORCHID FAHRENHEIT    S3              NI        NI        NI
    VA/VLB
ORCHID PRODESIGNER 2 ET4000     NI   NI   NI   NI    B    B
ORCHID PRODESIGNER   ET4000     NI   NI   NI   NI    B    B
    IIS
PARADISE WINDOWS     WD         NI   NI   NI   NI    B    B
    GRAPHICS ACCELERATOR
STB POWERGRAPH X-24  S3              NI        NI        NI
STB POWERGRAPH       S3              NI        NI        NI
    VL-24
STB WIND/X HC        S3              NI        NI        NI
TRIDENT 8900C        TRIDENT    NI   NI   NI   NI    B    B
TRIDENT 9000         TRIDENT    NI        NI         B
VIDEO SEVEN ®      VIDEO7     NI   NI   NI        NI
    VRAM
VIDEO SEVEN VRAM II  VIDEO7     NI   NI   NI   NI   NI   NI
 
Common modes in table above  Other Resolutions
---------------------------  -----------------
NI  Non-Interlaced           1 640x400x256  5  800x60065k    9 1152x900x256
 I  Interlaced               2 640x480x65k  6  800x600x16m   10
1152x900x65k
 B  Both Interlaced          3 640x480x16m  7  1024x768x65k  11
1280x1024x256
    and Non-Interlaced       4 640x480,     8  1040x768x256
                                 true color
 
Display adapters not listed above are expected to work if they use the
following supported chip sets. Install first as Standard VGA, then
select the corresponding driver from the Setup application in Program
Manager.
 
Chip Set                            Driver
--------------------------------    --------------------------------
ATI Mach 8                          ATI
ATI Mach 32                         ATI
ET4000                              ET4000
S3 801, 805, 911, 911A, 924, 928    S3
WD90C30                             Western Digital/Paradise
WD90C31                             Western Digital/Paradise
VGA                                 VGA
 
The following table shows the maximum display and color resolutions
available with each video driver using different amounts of video RAM.
Most display adapters can use the standard VGA driver for 16-color
modes.
 
                 Video                    Colors                    True
Drivers           RAM      16         256        65k       16m      Color
---------------  -----  ---------  ---------  ---------  ---------  -------
ATI              1Mb               1024x768    640x480   640x480
                 2Mb               1280x1024  1024x768   800x600    640x480
Cirrus           1Mb    1024x768   1024x768
COMPAQ AVGA      512Kb   800x600    640x480
COMPAQ Qvision   512Kb              640x480
                 1Mb               1024x768
                 2Mb               1280x1024
DGX              2Mb               1280x1024  1152x900
ET4000           512Kb  1024x768    640x480
                 1Mb    1024x768   1024x768
NCR 77C22        1Mb    1024x768   1024x768
S3               1Mb               1024x768
                 3Mb               1280x1024
Trident          512Kb  1024x768
                 1Mb    1024x768   1024x768
Video7           512Kb  1024x768    640x480
                 1Mb    1024x768   1024x768
VGA              256Kb   640x480
                 512Kb   800x600
WD               1Mb    1024x768   1024x768
XGA              1Mb               1040x768
 
Network Adapters
================
 
The following network adapters have been tested.  Adapters listed with
* have been tested for use with both x86 and MIPS platforms.
 
*3Com 3C503 EtherLink II ® (Coax & TP)
*3Com 3C503/16 EtherLink II/16 (Coax & TP)
*3Com 3C507 EtherLink ® 16 (Coax & TP)
*3Com 3C509 EtherLink III Parallel Tasking Adapter - ISA (Coax, TP and
Combo)
3Com 3C523 EtherLink/MC (Coax & TP)
3Com 3C529 EtherLink III Parallel Tasking Adapter - MCA (Coax & TP)
*3Com 3C579 EtherLink III Parallel Tasking Adapter - EISA (Coax & TP)
Advanced Micro Devices Am1500T Ethernet Adapter
Advanced Micro Devices Am2100 Ethernet Adapter
Advanced Micro Devices PCnet
Advanced Micro Devices PCnet-ISA Single Chip Ethernet Controller
*COMPAQ 32-Bit Dualspeed Token Ring Controller
COMPAQ 32-Bit Netflex Controller
COMPAQ 32-Bit Netflex Controller with Token Ring Module
COMPAQ Ethernet 16TP Controller
COPS LTI ISA
*DEC DE100 EtherWORKS LC
*DEC DE101 EtherWORKS LC/TP
*DEC DE200 EtherWORKS Turbo
*DEC DE201 EtherWORKS Turbo/TP
*DEC DE202 EtherWORKS Turbo TP/BNC
*DEC DE422 EtherWORKS EISA TP/BNC
*IBM Token Ring Adapter 16/4
IBM Token Ring Adapter 16/4 /A
Intel EtherExpress [TM] 16 MCA PCLA8110
Intel EtherExpress 16 MCA TP PCLA8120
*Intel EtherExpress 16 PCLA8110
*Intel EtherExpress 16C PCLA8100
*Intel EtherExpress 16TP PCLA8120
*Intel EtherExpress FlashC PCLA8105
National Semiconductor DP83932 (SONIC) Motherboard Ethernet Controller
   on MIPS ARC/R4000 systems
*Network Peripherals NP-EISA/S FDDI
Network Peripherals NP-MCA/S FDDI
Novell/Eagle Technology NE1000
*Novell/Eagle Technology NE2000
*Novell/Eagle Technology NE3200
*Proteon ProNET-4/16 p1390 ISA Adapter
Proteon ProNET-4/16 p1990 EISA Adapter
*Standard Microsystems 8003EP EtherCard PLUS
*Standard Microsystems 8013EBT EtherCard PLUS16
*Standard Microsystems 8013EP EtherCard PLUS Elite16
Standard Microsystems 8013EP/A EtherCard PLUS Elite/A
*Standard Microsystems 8013EPC EtherCard ® PLUS Elite16
*Standard Microsystems 8013EW EtherCard PLUS EliteCombo
*Standard Microsystems 8013EWC EtherCard PLUS EliteCombo
*Standard Microsystems 8013W EtherCard PLUS Elite16T
*Standard Microsystems 8013WB EtherCard PLUS
*Standard Microsystems 8013WC EtherCard PLUS Elite16T
Standard Microsystems 8013WP/A EtherCard PLUS Elite10T/A
Ungermann-Bass NIUpc
*Ungermann-Bass NIUpc/EOTP
Ungermann-Bass NIUps/EOTP
 
Multimedia Audio Adapters
=========================
 
The following audio adapters have been tested.
 
COMPAQ Business Audio
Creative Labs Sound Blaster [TM] 1.x
Creative Labs Sound Blaster Pro [39]
Media Vision Pro AudioSpectrum-16 [40]
Media Vision Pro AudioStudio [40]
Media Vision Thunder Board [39]
Microsoft Windows [TM] Sound System
 
Built-in audio adapter on MIPS ARC/R4000 systems.
 
Modems
======
 
The following modems are supported for use with Remote Access
Services.
 
ATI 2400 etc/e
ATI 9600 etc/e
AT&T ® 2224 CEO
AT&T Comsphere 3810
AT&T Comsphere 3811
AT&T Comsphere 3820
AT&T Comsphere 3830
AT&T Dataport
AT&T 4024
Bocamodem M1440
Cardinal 2400e
Cardinal 9600
Cardinal 14400
Cardinal 14400 Internal
Codex 2264
Codex 3220
Codex 3260
Codex 3261
Codex 3262
Codex 3263
Codex 3265
Codex 3260 Fast
Codex 3261 Fast
Codex 3262 Fast
Codex 3263 Fast
Codex 3265 Fast
Codex 3220 Plus
CXR Telcom 1445
DataRace RediModem V.32bis [41]
Datatrek 2424AMH
Datatrek Elite 624D [42]
Datatrek V.32 [43]
Digicom Scout
Digicom Scout Plus
DSI 9624LE Plus
DSI 9624E
ETech UFOMATE P1496MX
Evercom 24
Evercom 24E
Evercom 24E+
Gateway 2000 Telepath Internal
GVC SM2400
GVC SM96
GVC FM14400
Hayes ® Compatible 1200
Hayes Compatible 2400
Hayes Compatible 9600
Hayes Pocket Modem 2400
Hayes Smartmodem [TM] 2400
Hayes Smartmodem 9600
Hayes Optima 9600
Hayes Optima 14400
Hayes Ultra 9600
Hayes Ultra 14400
Hayes V Series 9600
Intel SatisFaxtion ® 100
Intel SatisFaxtion 400e
Intel 9600EX
Intel 14400EX
Macronix Maxlite Fax 9696
Macronix VOMAX 2000
Megahertz P2144 Pocket Faxmodem
Megahertz T3144 for Toshiba
Megahertz Z3144 for Zenith
Megahertz C5144 for COMPAQ LTE
MicroCom QX ® 4232bis [42]
MicroComQX 4232HS
MicroGate MG96 [41]
MicroGate MG144 [41]
MicroPorte 1042
MultiTech MultiModem 224 [44]
MultiTech MultiModem MT932
NEC 9635E Plus
Octocom 8324 [41]
Octocom 8396
PDI-1000 [43]
Practical Peripherals 2400 Pocket
Practical Peripherals 2400SA [43]
Practical Peripherals 2400MNP [42]
Practical Peripherals 9600SA
Practical Peripherals 14400SA
Racal-RMD 2412
Racal-RMD 2412/2 [45]
Racal-RMD 3221
Racal-RMD 3222
Racal-RMD 3226
Racal-RMD 3223
Racal-RMD 9632PA
Racal-RMD 9642PA
SupraModem 2400
Supra Fax Modem 9624 Internal
Supra Fax Modem V32
Supra Fax Modem V32bis
Supra Fax Modem Plus
Telebit ® QBlazer
Telebit T1000
Telebit T1500 [43]
Telebit T1600 [42]
Telebit T2000
Telebit T2500
 
Telebit T3000
Telebit TrailBlazer ® Plus
Telebit WorldBlazer
Telebit WorldBlazer-Rackmount
UDS Motorola ® V.3225 [42]
UDS Motorola V.3227 [46]
UDS Motorola V.3229
UDS Motorola FasTalk V.32/42b [46]
US Robotics Courier Dual
US Robotics Courier HST
US Robotics Courier V.32bis
US Robotics Sportster 2400
US Robotics Sportster 9600
US Robotics Sportster 14400
Ven-Tel 9600 Plus II [47]
Ven-Tel Pocket 24 V.42bis FAX
Ven-Tel 14400 Fax
Ven-Tel 14400 Fax Internal
Western Datacom Worldcom V32bis [43]
Zoom AFX
Zoom FX 9624V
Zoom VFX V.32bis
ZyXel U-1496
ZyXel U-1496E
 
Hardware Security Hosts
=======================
 
The following hardware security hosts have been tested for use with
Remote Access Services.
 
Digital Pathways Defender 1000D
Racal Gaurdata GSM
Security Dynamics ACM400
 
ISDN Adapters
=============
 
The following ISDN adapters have been tested for use with Remote
Access Services.
 
DigiBoard PCIMAC ISA Adapter
DigiBoard PCIMAC MC Adapter
DigiBoard PCIMAC/4 Adapter
 
Technical Notes
---------------
 
Items listed with ++ are supported with device drivers available in the
Windows NT Driver Library.
 
 1 Refer to SETUP.TXT for information on configuring this
   machine/device before installation.
 2 Only the NCR 53c710 SCSI Host Adapter is supported in this machine.
 3 Contact the manufacturer for information on running Windows NT on
   this machine.
 4 Tested with firmware revisions 3.10 and 3.20.
 5 This adapter requires an active terminator for proper performance.
 6 This adapter must be configured for 5 MB/second asynchronous I/O to
   work with listed CD-ROM drives from NEC.
 7 This adapter must be configured for 5 MB/second asynchronous I/O to
   work with listed CD-ROM drives from Chinon, Hitachi and NEC.
 8 Tested with the Unisys PW2 Advantage 3256 (Flemington).
 9 Tested with the Unisys PW2 Advantage Plus MPE 4668.
10 Removable media drives are not supported with cache module
   installed.
11 CD-audio, tape drives and scanners are not supported on this
   controller.
12 To use this adapter, at least one device on the bus must provide
   termination power.
13 Refer to SETUP.TXT for information on configuring this adapter.
14 SCSI BIOS dated before 1991 requires PS/2 Reference Diskette
   version 1.21 or later.
15 This adapter cannot be used for CD Setup. To install Windows NT
   with this adapter, use the WINNT.EXE Setup method.
16 Scanners are not supported with this adapter.
17 Tested with COMPAQ Portable 486c.
18 Tested with NCR System 3000 Model 3350.
19 This adapter is currently supported in its ESC-1/ESC-2
   compatibility mode only.
20 This adapter is a RAID controller which supports hard drives only.
21 This adapter is only supported on IRQ-5.
22 This adapter is only supported for use with scanners and CD-ROM
   drives.
23 Tested with firmware revision 005.
24 Tested with firmware revision 008.
25 Audio is not supported on this drive.
26 This drive is not supported for use with the Adaptec AHA-1542c.
27 This drive requires double-termination when used with the Adaptec
   AHA-1742A.
28 This drive is not supported for use with the Future Domain TMC-850M
   and TMC-1670 adapters.
29 The Adaptec AHA-1640 and Ultrastor 24f support only a single disk
   when used with this drive. This drive is not supported for use with
   the Future Domain MCS-600 adapter.
30 Requires firmware revision 1.10C to function properly with Windows
   NT.
31 This drive is not supported with the Adaptec AHA-1640 adapter.
32 This drive is not supported with the IBM PS/2 Microchannel SCSI
   Host Adapter (with cache).
33 This drive is not supported with the Future Domain TMC-850M(ER).
34 This drive is not supported with the Adaptec AHA-1742A adapter.
35 This drive is not supported with the UltraStor 24fa adapter.
36 For use with floppy controllers. Separate interface controllers for
   these types of drives are not supported.
37 Requires that 512-byte sector-sized media be mounted during
   installation.
38 Tested with HP C2225B tape drive, HP C2229B disk drive and HP
   C2226A CD-ROM drive.
39 Supported in Sound Blaster 1.x compatibility mode.
40 Not supported in Sound Blaster 1.x compatibility mode.
41 Error control and flow control forced on.
42 Advanced features disabled.
43 Supported as a client modem only.
44 Flow control forced on.
45 Maximum DTE speed set to 2400.
46 Maximum DTE speed set to 9600.
47 Modem compression forced on.
48 In the UPS applet, check the box "Remote UPS Shutdown" and set it
   to high.
 
Additional reference words: prodnt 3.10 HCL
KBCategory: kbhw
KBSubCategory: nthw HCLIST
 
=============================================================================
 
Copyright Microsoft Corporation 1995.
