Knowledge Base |

# Bookshelf Atlas Map Printed on LaserJet III/IIISi Is Dithered

Article ID: 123201

Article Last Modified on 11/15/2006

APPLIES TO

- Microsoft Windows 95

This article was previously published under Q123201

## SYMPTOMS

When you print a selected map from the Microsoft Bookshelf '94 Atlas to a Hewlett-Packard (HP) LaserJet III or IIISi, the printed map appears to contain dots or dithering. These dots do not occur when you print from Windows version 3.1.

## CAUSE

The Windows 95 Universal Printer Driver dithering option is set to a value other than None.

## RESOLUTION

To print a non-dithered map, set the Windows 95 dithering option for the HP LaserJet III or IIISi to None. To change the dithering option, perform the following steps:

1. Click the Start button, point to Settings, and then click Printers.
2. Use the right (secondary) mouse button to select the HP LaserJet III or IIISi printer.
3. Click Properties, then click the Graphics tab.
4. Under Dithering, click None.
5. Click OK.

## MORE INFORMATION

This behavior is caused by changes in the Windows 95 printing system. With the Windows 3.x HP printer driver, GDI.EXE is given a non-dithered bitmap to stretch; with the Windows 95 Universal Printer Driver, GDI.EXE is given a dithered bitmap to stretch, which results in the dithering pattern.

Additional query words: spots dots dotted 3rdparty laser jet

Keywords: KB123201