Knowledge Base |

# Maynard 16 Bit ISA SCSI Adapter is Hard-Coded IRQ 10 and DMA 5

Article ID: 104577

Article Last Modified on 4/9/2004

APPLIES TO

- Microsoft Windows NT Advanced Server 3.1
- Microsoft Windows NT Workstation 3.1
- Microsoft Windows NT Advanced Server 3.1

This article was previously published under Q104577

## SUMMARY

The Maynard 16-Bit ISA SCSI adapter is hard coded to use IRQ 10 and DMA channel 5. It is not possible to modify these settings. If another device in the computer is configured for either of these settings, your computer may be unable to boot Windows NT. If this is the case, change the settings on the other device.
Maynard Electronics is owned by Conner Peripherals. For additional information, contact Conner technical support at (800) 227-6296.
The Maynard SCSI adapter is manufactured by Maynard Electronics, a vendor independent of Microsoft; we make no warranty, implied or otherwise, regarding this products' performance or reliability.

Additional query words: prodnt

Keywords: kbhardware KB104577