Knowledge Base |

# Maximum of 5 Domains Can be Viewed with LAN Manager

Article ID: 102627

Article Last Modified on 10/31/2006

This article was previously published under Q102627

## SUMMARY

You can monitor no more than five LAN Manager domains. Using the LAN Manager setup program you can specify one default (logon) domain name and four different entries for otherdomains.
In the LANMAN.INI file you can find values for the following two keys in the section [workstation]:

         [workstation]
         ...
         DOMAIN     = <default_domain_name>
         OTHDOMAINS =
    <domain_name1>,<domain_name2>,<domain_name3>,<domain_name4>
         ...

Additional query words: 2.00 2.10 2.10a 2.20 2.0 2.1 2.1a 2.2

Keywords: KB102627