Hardware Failure Errors with RAS & US-Robotics 14400 Sportster

PSS ID Number: Q111093
Article last modified on 05-13-1994

3.11
WINDOWS

---------------------------------------------------------------------
The information in this article applies to:

 - Microsoft Windows for Workgroups version 3.11
---------------------------------------------------------------------

Microsoft does not encourage nor support user changes to .INF files;
therefore, Microsoft Product Support Services (PSS) does not support the
procedure in this article. Although we have tested the following procedure
and it appears to function as described; we strongly recommend that you
make a backup copy of your .INF file before you proceed.

SYMPTOMS
========
When you use Remote Access Services (RAS) with a US-Robotics Internal 14400
Sportster, you receive the following error messages:
   Error 692: Hardware Failure in attached port or device

RESOLUTION
==========
To correct this problem, edit the modem initialization entry
(COMMAND_INIT=) in the [US Robotics Sportster 14400] section of the
MODEM.INF file. To do so:
1. Run Microsoft Windows for Workgroups Write and open the MODEM.INF file.
2. Choose the No Conversion button.
3. From the Find menu, choose Find.
4. In the Find What box, type "[US Robotics Sportster 14400]" (without the
   quotation marks) and then choose Find Next.
5. Choose Cancel and then change "AT&F" to "ATZ&F" (without the quotation
   marks). For example, change
      COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W1 S95=44
   to:
      COMMAND_INIT=ATZ&F&C1&D2 V1 S0=0 S2=128 S7=55 W1 S95=44
6. Save the MODEM.INF file.
7. Quit and restart RAS Phonebook.
This issues a reset command first, and then resets the modem to the factory
defaults.

Additional reference words: 3.11 string
=============================================================================
Copyright Microsoft Corporation 1994.