Knowledge Base |

# Add Line to PROTOCOL.INI to Load TCP/IP with Madge Card

Article ID: 100542

Article Last Modified on 7/30/2001

This article was previously published under Q100542

## SUMMARY

When loading TCP/IP with the Madge card, be sure to add autoopen=no to PROTOCOL.INI. This option is not clearly stated in the LAN Manager documentation, and does not appear in the MS-DOS ini section. The default value is YES, but TCP/IP needs the OpenAdapter and CloseAdapter functions from the NIC driver (by means of PROTMAN).

Additional query words: adapter 2.00 2.0 2.10 2.1 2.10a 2.1a 2.20 2.2

Keywords: KB100542