Knowledge Base |

# Port Trapping in Windows 3.0/3.1

Article ID: 100947

Article Last Modified on 8/30/2004

APPLIES TO

- Microsoft Windows Software Development Kit 3.0
- Microsoft Windows Software Development Kit 3.1

This article was previously published under Q100947

## SUMMARY

In enhanced mode Windows, the I/O permission bitmap (IOPM) is used by the virtual machine manager (VMM) to determine whether I/O is permitted at a given I/O port. The IOPM is clear when the VMM is initialized, which means that any I/O port can be accessed. VxDs can trap specific I/O ports to prevent direct access. Therefore, unless a VxD traps a port, direct I/O access is permitted. In standard mode, the IOPM is not used, so direct I/O access is always permitted. This does not apply to Windows NT.
The sample IOPORT.ZIP lists ports trapped by the standard VxDs included in enhanced mode Windows (IOPMPORT.XLS and IOPMPORT.TXT), and an MS-DOS program IOPM.EXE, which lists all currently trapped ports. Also, the DT (dump TSS) command in WDEB386 lists all currently trapped ports.

## MORE INFORMATION

The following files are available for download from the Microsoft Download Center:
Ioport.exe
For additional information about how to download Microsoft Support files, click the following article number to view the article in the Microsoft Knowledge Base:

119591 How to Obtain Microsoft Support Files from Online Services

Microsoft scanned this file for viruses. Microsoft used the most current virus-detection software that was available on the date that the file was posted. The file is stored on security-enhanced servers that help to prevent any unauthorized changes to the file.
The IOPM is contained in the task state segment (TSS). The I/O privilege level (IOPL) and the I/O permission bitmap determine whether a task is allowed to perform I/O. The IOPL determines the minimum privilege level required to perform I/O without checking the permission bitmap. For example, if IOPL = 1, then a procedure must have a code privilege level (CPL) of 1 or 0 (zero) to perform unrestricted I/O. However, if the CPL of the current task is greater than the IOPL, or the processor is operating in virtual 8086 mode, then the I/O permission bitmap is checked to determine whether I/O is permitted at the requested port.
In enhanced mode Windows, CPL is always greater than IOPL, so the IOPM is always checked to determine whether direct I/O access is permitted. In standard mode, CPL equals IOPL, so the IOPM is never checked.
Each bit in the bitmap corresponds to an I/O port byte address. For example, the bit for port address 60 (decimal) corresponds to the 60th bit, or the 4th bit in the 8th byte of the bitmap. In enhanced mode Windows, the bitmap is always 8192 bytes, and the bitmap is initialized to allow I/O at any port.
When a VxD is initialized, it can call Install_IO_Handler to trap specific I/O ports. Install_IO_Handler sets the corresponding bits in the IOPM. When a trapped port is accessed, the VxD I/O handler will take over and perform the appropriate action. Windows maintains a single TSS for all VMs. When a VM switch occurs, the TSS IOPM is updated to reflect the local IOPM of the incoming VM. Port trapping for a specific port may be disabled locally or globally from a VxD by calling Disable_Local_Trapping or Disable_Global_Trapping.

Additional query words: softlib IOPORT.ZIP kbfile

Keywords: kb16bitonly kbfile kbsample KB100947