# README.TXT: Patch 44 for SNA Server 2.0

ID: Q115383

###

The information in this article applies to:

- Microsoft SNA Server for Windows NT, version 2.0

The following is the README.TXT file that accompanies SNA Server 2.0 patch 44 (SNA20.P44):

Note that this article reflects the text of a static document. Therefore, some of the information in this article may be outdated. For example, as of May 20, 1996, Microsoft no longer maintains support forums on CompuServe.

******************* Beginning of Readme ***************************

Product: Microsoft SNA Server for Windows NT v2.0 Update: Patch #44 (includes patch #30) Status: Confirmed

PKZIP 2.04g format -- uncompress using the "-d" option.

Date: May 9, 1994

Modules updated:

    \SYSTEM\SNADLC.DLL   05/08/94  09:36p  74752

\SYSTEM\HWSETUP\SNADLC\SNADLC.DLL (same file)

Bugs fixed:

2058 SNALINK application exception in 802.2 link service.

Under stress, the SNA Server 802.2 link service may fail with an application exception. Looking at the drwtsn32.log, the failure occurred in routine "sbpa4s", caused by an uninitialized variable

1985 SNA Server DLC timers not optimally configured (Patch #30)

Ensure that t1, t2, and ti timers configured for an SNA Server 802.2 connection defaults are configured optimally within the configuration file.

Update Procedure:

- Stop the SNA Server service

- Copy the new SNADLC.DLL to the above locations on the server.

*********************** End of Readme *******************************

SNA Server 2.0 patches are located on:

- Library #2 of the MSSNA Compuserve forum.
- The Internet server under BUSSYS\SNASRVR\SUP-ED\FIXES\ (supported patches) OR on BUSSYS\SNASRVR\UNSUP-ED\FIXES\ (unsupported patches).

Additional query words: prodsna

    Keywords          : kbnetwork ntdistrib
    Version           : 2.0
    Platform          : WINDOWS

Last Reviewed: April 18, 1997