Knowledge Base |

# MediaVision SCSI Adapter Supports Devices on Windows NT HCL

Article ID: 104747

Article Last Modified on 11/1/2006

APPLIES TO

- Microsoft Windows NT Advanced Server 3.1
- Microsoft Windows NT Workstation 3.1

This article was previously published under Q104747
MediaVision, which manufactures the ProAudio Spectrum 16 (PAS16) sound card, distributes a list of CD-ROM drives that have been tested and certified as compatible with the ProAudio Spectrum's on-board Trantor SCSI controller. This list is specific to the MS-DOS Trantor SCSI driver (TSLCDR.SYS) distributed by MediaVision.
According to Trantor Systems, the manufacturer of the controller on the PAS16, if you use the Trantor MediaVision SCSI driver provided with Windows NT (TMV1.SYS), the PAS16 SCSI controller should support any SCSI device that is on the Windows NT Hardware Compatibility List (HCL).
NOTE: A CD-ROM device that is listed by MediaVision as tested and compatible with the PAS16 does not necessarily imply that it will work under Windows NT.

## MORE INFORMATION

The PAS16 automatically provides termination for its end of the SCSI bus. However, it may be necessary to configure the CD-ROM drive (or the last device on the bus) to terminate the other end.
The PAS16 reserves SCSI ID #7 by default. (This cannot be changed.) Any other SCSI ID number (0-6) can be used with the CD-ROM drive or other SCSI devices. For additional information, contact MediaVision technical support at (800) 638-2807 or (510) 770-9905.
The products included here are manufactured by MediaVision, Inc., a vendor independent of Microsoft; we make no warranty, implied or otherwise, regarding this product's performance or reliability.

Additional query words: prodnt

Keywords: kbhardware KB104747