PCMCIA Cards Detected Twice on IBM ThinkPad 750 and 750c
  
PSS ID Number: Q119091
Article last modified on 08-22-1995
 
95
 
WINDOWS
 

---------------------------------------------------------------------
The information in this article applies to:
 
 - Microsoft Windows 95 Preview Program
---------------------------------------------------------------------
 
SYMPTOMS
========
 
On the IBM ThinkPad 750 and 750C, PCMCIA cards are reported as two separate
nodes under the Device Manager card class.
 
CAUSE
=====
 
When the Socket Services driver attempts to determine the number of PCMCIA
sockets in the ThinkPad, the ThinkPad incorrectly reports that there are
more than two PCMCIA sockets, even though the ThinkPad has only two.
 
WORKAROUND
==========
 
To work around this problem:
 
1. Click the Start button, point to Settings, then click Control Panel.
 
2. Double-click the System icon, and then click the Device Manager tab.
 
3. Expand the PCMCIA Socket branch and click "Intel PCIC Compatible PCMCIA
   Controller."
 
4. Click the Properties button, then click the Socket Services tab.
 
5. In the Number Of Sockets box, change the value from Automatic Detection
   to 2.
 
6. Click Apply Now on all open property sheets, then click Shut Down on the
   taskbar and restart Windows 95.
 
Now any PCMCIA card you plug in will be detected only once.
 
If you already have two instances of a PCMCIA device in Device Manager,
select the class of the card (for example, Modem or Network), expand the
branch and remove one of the instances of that device.
 
MORE INFORMATION
================
 
The products included here are manufactured by vendors independent of
Microsoft; we make no warranty, implied or otherwise, regarding these
products' performance or reliability.
 
KBCategory: kbhw kb3rdparty kbprb kbsetup
KBSubcategory: wpp95 win95
Additional reference words: 95 3rdparty
 
=============================================================================
 
Copyright Microsoft Corporation 1995.
