Knowledge Base |

# Network DDE Applications Fail with TCP/IP-32

Article ID: 120122

Article Last Modified on 10/13/2003

APPLIES TO

- Microsoft TCP/IP for Windows for Workgroups 3.11
- Microsoft Windows for Workgroups 3.11

This article was previously published under Q120122

## SYMPTOMS

Network DDE Windows-based applications (like File Manager) fail to operate successfully between Windows for Workgroups workstations configured with TCP/IP-32 when they are in different sub-nets connected by routers. The following error message appears:
The computer name specified in the network path cannot be located
You can observe workstations with a protocol analyzer. Unsuccessful Name Query requests broadcasted to the local sub-net are transmitted by workstations to resolve the name of the workstation in question: "computername <1F>".
The NET USE command functions correctly.

## CAUSE

The NetBIOS naming table on the workstation does not include the name required by Network DDE for computer names specified in the LMHOSTS file. This problem only occurs under TCP/IP-32 if you use the #PRE keyword.
When a name entry is parsed from the LMHOSTS file, three entries are added to the workstation's NetBIOS naming table. These are added to provide the computer name, messenger, and server functionality:

       computername   00h
       computername   20h
       computername   03h

## RESOLUTION

### TCP/IP-16 Real Mode

Use the ADDNAME2 keyword available from the LAN Manager resource kit. The following syntax adds an additional entry which can then be saved to the LMHOSTS file:

       addname2 "computername   " /p0x1f

The entire length of the name must be 16 characters including the hidden character (1f) in the 16th place. You must pad the computer name with spaces so that it equals 15 characters in length.

### TCP/IP-32 for Windows for Workgroups 3.11

TCP/IP-32 can add the required NetBIOS name (if you are using the #PRE keyword) by having the two following lines in the LMHOSTS file of each remote computer:

       ipaddr computername #PRE
       ipaddr "COMPUTERNAME   \0x1F" #PRE

NOTE: The computer name in quotation marks on the second entry must equal 16 characters in length, and it must be in uppercase. The #PRE keyword is optional for the second entry above. #PRE speeds up resolution of the Network DDE name which helps to provide a successful connection accross routers providing a dialup or delayed remote link.

Additional query words: wfw wfwg prodtcp32 1.0 NetDDE Chat LMhosts kbbug1.00

Keywords: KB120122