Knowledge Base |

# Installing LapLink Version 6.0b for Windows Causes GP Fault

Article ID: 121445

Article Last Modified on 1/19/2007

APPLIES TO

- Microsoft Windows 98 Second Edition
- Microsoft Windows 98 Standard Edition
- Microsoft Windows 95

This article was previously published under Q121445
If this article does not describe your hardware-related issue, please see the following Microsoft Web site to view more articles about hardware:

http://support.microsoft.com/default.aspx/w98?sid=460

## SYMPTOMS

After you install LapLink version 6.0b for Windows in Windows 95, you may receive a general protection (GP) fault error message when you restart your computer.

## CAUSE

This problem occurs if you upgrade LapLink version 6.0 or 6.0a for Windows to version 6.0b. LapLink 6.0b for Windows removes the previous LapLink drivers and then prompts you to restart your computer and run Setup again. When you restart your computer, a GP fault occurs and you cannot continue.

## RESOLUTION

To install LapLink 6.0b for Windows, follow these steps:

1. Restart your computer in Safe mode. To do so, restart your computer, press the F8 key when you see the "Starting Windows 95" message, and then choose Safe Mode from the Startup menu.
2. Run LapLink's Uninstall program. To do so, click the Start button, point to Programs, click LapLink For Windows, and then click Uninstall.
   NOTE: If you installed LapLink for Windows in a group named something other than LapLink For Windows, click that name instead.
3. After the LapLink Uninstall program is finished, reselect your video adapter driver. To do so, follow these steps:
   1. In Control Panel, double-click the Display icon.
   2. On the Settings tab, click Change Display Type.
   3. Note the adapter type listed in the Adapter Type box, and then click Change in the Adapter Type area.
   4. In the Models box, click the adapter type you noted in step C, and then click OK.
   5. Click OK or Close until you return to Control Panel.
   6. When you are prompted to restart your computer, do so. Let Windows 95 start normally.
4. Install LapLink 6.0b for Windows.

NOTE: You cannot install LapLink for Windows if you are using a Number Nine Imagine 128 video adapter. For information about a possible work- around for this problem, please contact Number Nine.

## MORE INFORMATION

To use animated cursors with LapLink installed in Windows 95, you must use LapLink 6.0b. Earlier versions of LapLink cause animated cursors to turn black and not animate.
For information about known issues that can occur after you install LapLink for Windows, please obtain document number 5521 from Traveling Software's FaxBack service.
LapLink for Windows is manufactured by Traveling Software, Inc., a vendor independent of Microsoft; we make no warranty, implied or otherwise, regarding this product's performance or reliability.

Additional query words: HWDISEM gpf #9 llw

Keywords: kbappcompatibility kbprb KB121445