Hardware Compat. List: x86 Computers (T-Z) - SCSI Tape Drives
  
PSS ID Number: Q101575
Article last modified on 09-16-1994
 
3.10
 
WINDOWS
 

----------------------------------------------------------------------
The information in this article applies to:
 
 - Microsoft Windows NT operating system version 3.1
----------------------------------------------------------------------
 
T-DATA LIN 486-33 DX
T-DATA LIN 486-50 DX
Tandon 486dx/33
Tandon 486dx2/66
Tandon MCSII 486dx/33
Tandon MCSII 486dx/33c
Tandon MCSII 486dx2/66c
Tandon NII 486dx/33
Tandon PACII plus 486dx2/66
Tandon PCAII 486dx2/66
Tandon PCAII 486sx/25
Tandon Profile 486dx/33
Tandon TargetII 486dx2/66
Tandon TargetII 486sx/25
Tandon Tower 486dx/66e
Tandon TowerII 486dx2/66
Tandy ® 425 SX
Tandy 433 DX
Tandy 433 SX
Tandy 450 DX2
Tandy 466 DX2
Tandy 4820 SX/T
Tandy 4825 SX
Tandy 4833 LX/T
Tandy 4850 EP
Tandy 4866 LX/T
Tangent 486DX/33 EISA
Tangent 486DX/33 ISA
Tatung TCS-8460S 386SX/25
Tatung TCS-9300T 486DX2/66
Tatung TCS-9360T 486DX/33
Tatung TCS-9370T 486DX2/66
Tatung TCS-9620E 486DX2/66
Tatung TCS-9650E 486DX2/66
Tatung TCS-9700 486DLC/40
Tatung TCS-9910S 486SLC/33
Techway Endeavour E62
Techway Endeavour E62VL
Techway Endeavour E77
Techway Endeavour E77VL
Techway Endeavour E84
Techway Endeavour E84VL
TELEMECANIQUE FTX507-6B
Texas Instruments TravelMate [TM] 4000 Color Series [1]
Texas Instruments TravelMate 4000 Series [1]
Texas Instruments TravelMate 4000 WinDX2 [1]
TFE Atlantic 486 DX 50MHz
Tiki-Data PC UNIVERSAL
Toshiba ® T4400SX
Toshiba T4500
Toshiba T6400SX
Tri-Star TriCAD 486/66
Tri-Star Tri-Win Station
TriGem 486/33MM (incl. 486 /P (Type 30) model)
TriGem 486/50F
TriGem 486/66F
TriGem 486/66VC
TriGem 486DX2/50MM (incl. 486 /P (Type 40)
TriGem 486DX2/66MM (incl. 486 /P (Type 50) model)
TriGem 486VC
TriGem 4DX/33ME
TriGem 4DX2/50ME
TriGem 4DX2/66ME
TriGem 4SX/25ME
TriGem 4SX/33ME
TriGem SX486/25C
TriGem SX486/25MM (incl. 486 /P (Type 10 and 12) models)
TriGem SX486/33MM (incl. 486 /P (Type 20) model)
Tulip ® Vision Line DT/DC 486DX-33i
Tulip Vision Line DT/DC 486DX-50i
Tulip Vision Line DT/DC 486DX-66i
Tulip Vision Line series 486DX-33i
Tulip Vision Line series 486DX-50i
Tulip Vision Line series 486DX-66e
Tulip Vision Line Series 486DX-66i
TWINHEAD Superset 700
U.S. Micro Jet 386-33
U.S. Micro Jet 386-40
U.S. Micro Jet 486-33
U.S. Micro Jet 486-50
U.S. Micro Jet 486DLC-33
U.S. Micro Jet 486DX2-50
U.S. Micro Jet 486DX2-66
U.S. Micro Jet 486SX-25
U.S. Micro Jet EISA 486-33
U.S. Micro Jet EISA 486-50
U.S. Micro Jet EISA 486DX2-50
U.S. Micro Jet EISA 486DX2-66
U.S. Micro Jet EISA 486SX-25
U.S. Micro Jet VL 486-50
U.S. Micro Jet VL 486DX2-50
U.S. Micro Jet VL 486DX2-66
U.S. Micro Jet VL 486SX-25
U.S. Micro Jet VL486-33
Ultra-Comp 486DX-33
Ultra-Comp 486DX-33 EISA VLB
Ultra-Comp 486DX-33 VLB
Ultra-Comp 486DX-50
Ultra-Comp 486DX-50 EISA VLB
Ultra-Comp 486DX-50 VLB
 
Ultra-Comp 486DX2-66
Ultra-Comp 486DX2-66 EISA VLB
Ultra-Comp 486DX2-66 VLB
Unidata 486 66 MHz ISA
Unisys ® PW2 3336
Unisys PW2 Advantage 3256
Unisys PW2 Advantage 3336
Unisys PW2 Advantage 4163
Unisys PW2 Advantage 4253
Unisys PW2 Advantage 4256
Unisys PW2 Advantage 4336
Unisys PW2 Advantage 4506
Unisys PW2 Advantage Plus 4668
Unisys PW2 Advantage Plus 5606
Unisys PW2 Advantage Plus 5608
Victor  DX/50
Victor 400 DX/50
Victor 400 SX/25
Victor 486 DX/66
Victor 486DX/33
Victor V486DSX/25
Viglen Contender 4DX33
Viglen EX-Series
Viglen Genie 4DX66
Vobis 486 VC-HD 33
Vobis 486 VC-HD 50
Vobis 486 VIO 66
Vobis 486 VIO SX25
Vtech LASER 386 Ultra Slim
Vtech LASER 486DX/3 Desktop
Vtech LASER 486DX/3 Desktop (w/LBVGA)
Vtech LASER 486DX/3 Desktop (w/VLBUS)
Vtech LASER 486DX/3 Tower
Vtech LASER 486DX/3 Tower (w/VLBUS)
Vtech LASER 486DX2/4 Desktop
Vtech LASER 486DX2/4 Desktop (w/LBVGA)
Vtech LASER 486DX2/4 Desktop (w/VLBUS)
Vtech LASER 486DX2/4 Tower
Vtech LASER 486DX2/4 Tower (w/VLBUS)
Vtech LASER 486DX2/6 Desktop
Vtech LASER 486DX2/6 Desktop (w/LBVGA)
Vtech LASER 486DX2/6 Desktop (w/VLBUS)
Vtech LASER 486DX2/6 Tower
Vtech LASER 486DX2/6 Tower (w/VLBUS)
Vtech LASER 486SX/3 Desktop
Vtech LASER 486SX/3 Desktop (w/LBVGA)
Vtech LASER 486SX/3 Tower
Vtech LASER 486SX/3 Ultra Slim
Vtech LASER 486SX/3 Ultra Slim (w/LBVGA)
Vtech LASER 486SX/4 Desktop
Vtech LASER 486SX/4 Desktop (w/LBVGA)
Vtech LASER 486SX/4 Desktop (w/VLBUS)
Vtech LASER 486SX/4 Tower
Vtech LASER 486SX/4 Ultra Slim
Vtech LASER 486SX/4 Ultra Slim (w/LBVGA)
Vtech LASER LT322 Notebook
Vtech LASER LT421 Notebook
Vtech Platinum SMP
Wang Microsystems ASI-CPU-E266
Wang Microsystems DTE-33
Wang Microsystems PC 350/40C
Western 486V25SX VESA  LOCAL BUS
Western 486V33 DX  EISA
Western 486V33 DX ISA
Western 486V50 DX EISA
Western 486V50 DX ISA
Western 486V50 DX2 ISA
Western 486V66 DX2 EISA
Western 486V66 DX2 ISA
Wyle Laboratories Intel Xpress Deskside w/486DX-50MHz
Wyle Laboratories Intel Xpress DeskTop  w/486DX2-66MHz
Wyle Laboratories Intel Xpress DeskTop w/486DX-50MHz
Wyse ® Decision 386/40
Wyse Decision 386SX/25C
Wyse Decision 486/25
Wyse Decision 486/33
Wyse Decision 486/33E
Wyse Decision 486/33T
Wyse Decision 486DX2/50
Wyse Decision 486se-25SX
Wyse Decision 486se-33DX
Wyse Decision 486se-33SX
Wyse Decision 486se-50DX2
Wyse Decision 486se-66DX2
Wyse Decision 486si-25SX
Wyse Decision 486si-33DX
Wyse Decision 486si-33SX
Wyse Decision 486si-50DX2
Wyse Decision 486si-66DX2
Wyse Decison 386/25
Wyse Series 6000i Model 640
Wyse Series 6000i Model 645
Wyse Series 7000i Model 740
Zenith Data Systems Z-386/25
Zenith Data Systems Z-386/33E
Zenith Data Systems Z-386SX/20
Zenith Data Systems Z-425/SX
Zenith Data Systems Z-425S+
Zenith Data Systems Z-433/DX
Zenith Data Systems Z-450X+
 
Zenith Data Systems Z-486/33ET
Zenith Data Systems Z-486SX/20
Zenith Data Systems Z-486SX/25E
Zenith Data Systems Z-Note 425Ln
Zenith Data Systems Z-Server 425SE
Zenith Data Systems Z-Server 433DE
Zenith Data Systems Z-Server 450DE
Zenith Data Systems Z-Station 420SEh
Zenith Data Systems Z-Station 420SEn
Zenith Data Systems Z-Station 420Sh
Zenith Data Systems Z-Station 420Sn
Zenith Data Systems Z-Station 425Sh
Zenith Data Systems Z-Station 425Sn
Zenith Data Systems Z-Station 433DEh
Zenith Data Systems Z-Station 433DEn
Zenith Data Systems Z-Station 433Dh
Zenith Data Systems Z-Station 433SEh
Zenith Data Systems Z-Station 450XEh
Zenith Data Systems Z-Station 450Xh
Zenith Data Systems Z-Station 450Xn
Zenith/INTEQ Tempest Workstation/Server
Zenon Z-Dream IIII EISA/VESA 486DX/66
ZEOS ® 486DX/33CDT
ZEOS 486DX/33EISA
ZEOS 486DX/33ISA
ZEOS 486DX/50
ZEOS 486SX/20DT
ZEOS Freestyle 386SL 25
ZEOS Upgradable 486 DX/33 Cache
ZEOS Upgradable 486 DX2/66 Cache
ZEOS Upgradable 486 SX/33 Cache
ZEOS Upgradable EISA 486 DX2/66 Cache
ZEOS Upgradable Local Bus DX2-66
 
x86 Architecture Multiprocessor Computers
=========================================
 
The following multiprocessor systems have been tested.
 
ACER AcerFrame 3000MP 33 (Model 3255) [1]
ACER AcerFrame 3000MP 50 (Model 3257) [1]
ALR POWERPRO DMP 4/50
ALR POWERPRO DMP 4/66d
ALR PROVEISA DMP 4/33
ALR PROVEISA DMP 4/50D
ALR PROVEISA DMP 4/66D
AST Manhattan SMP 486/50
AST Manhattan SMP Pentium
COMPAQ Systempro/XL Dual 486/50
COMPAQ Systempro Dual 386/25
COMPAQ Systempro Dual 486/33
COMPAQ SystemPro Dual 486DX2/66
Corollary Extended C-bus 486DX2/66
ICL System Platform MX486/50
Micronics MPro 2000
NCR System 3000 Model 3360
NCR System 3000 Model 3450 [2]
NCR System 3000 Model 3550 [2,3]
Olivetti LSX5040
Sequent WinServer 1000 [3]
Sequent WinServer 1500 [3]
Sequent WinServer 3000 [3]
Sequent WinServer 5000 [3]
Siemens-Nixdorf PCE-4T/33 Dual
Siemens-Nixdorf PCE-4T/50 Dual
Wyse Series 7000i Model 740MP/33
Wyse Series 7000i Model 740MP/66
Wyse Series 7000i Model 760MP
 
MIPS ® ARC/R4000 Series Computers
===================================
 
The following RISC systems have been tested.
 
ACER ARC1
ACER Formula
Carrera R4000 [TM]
DESKStation Evolution RISC PC
MIPS ARCSystem Magnum SC-50
MIPS ARCSystem Magnum PC-50
MIPS Millenium SC-50
MIPS Millenium PC-50
Olivetti M700-10
NeTPower  RISCpc Series 100
 
SCSI ® Host Adapters
======================
 
The following SCSI adapters have been tested with the following
scanner, CD-ROM, tape, fixed and removable drives (except as noted):
ArchiveST 4000 DAT, CD-Technologies CD Porta-Drive T-3401, Hewlett-
Packard ScanJet IIc, NEC Intersect CDR-74, Micropolis 1924, Peripheral
Land Infinity 88, Procom Technology MCD-DS, Syquest 5110, Toshiba TXM-
3401, WangTek 5150es. Adapters listed with * have been tested for use
with both x86 and MIPS platforms.
 
Adaptec ® AHA-1510
*Adaptec AHA-1520
*Adaptec AHA-1522
*Adaptec AHA-1540B [4]
Adaptec AHA-1540C
*Adaptec AHA-1542B [4]
Adaptec AHA-1542C [5]
Adaptec AHA-1640
Adaptec AHA-1740 [6]
Adaptec AHA-1742 [6]
*Adaptec AHA-1740A [7]
*Adaptec AHA-1742A [7]
*Adaptec AHA-2740
*Adaptec AHA-2742
Adaptec AIC-6260 [8]
Adaptec AIC-7770 [9]
Always IN-2000
BusLogic BT-445S
*BusLogic BT-542B
BusLogic BT-545S
BusLogic BT-640A
BusLogic BT-646S
BusLogic BT-742A
*BusLogic BT-747S
COMPAQ Fast SCSI-2 Controller
COMPAQ 6260 SCSI-2 Controller
DPT PM2011b (incl. cache) [10]
DPT PM2012b (incl. cache) [10]
*Data Technology Corp. 3290
Data Technology Corp. 3292 [11]
Future Domain MCS-600
Future Domain MCS-700
Future Domain TMC-845 [12, 13]
*Future Domain TMC-850 [12, 13]
*Future Domain TMC-850M(ER) [13]
Future Domain TMC-860 [12, 13]
Future Domain TMC-860M [13]
Future Domain TMC-885 [12, 13]
Future Domain TMC-885M [13]
*Future Domain TMC-1650
Future Domain TMC-1660
*Future Domain TMC-1670
Future Domain TMC-1680
*Future Domain TMC-7000EX
IBM PS/2 Microchannel SCSI Host Adapter [14]
IBM PS/2 Microchannel SCSI Host Adapter (with cache) [14]
Maynard 16-bit SCSI Adapter [15, 16]
MediaVision Pro Audio Spectrum-16
NCR 53C700 SCSI Adapter
NCR 53C710 SCSI Adapter
NCR 53C90 SCSI Controller [17]
*NCR 53C94 SCSI Controller [18]
Olivetti ESC-1
Olivetti ESC-2
Olivetti EFP-2 [19, 20]
Trantor T-128 [12, 21, 13]
Trantor T-228 [12, 13, 15, 22]
Trantor T-130B [12, 21]
++Trantor T-348 MiniSCSI Plus
*UltraStor 14f [23]
*UltraStor 24f [24]
UltraStor 24fa
UltraStor 34f
UltraStor 124f [20]
 
SCSI CD-ROM Drives
==================
 
The following CD-ROM drives have been tested with the following
adapters: Adaptec AHA-1510, AHA-1542C, AHA-1640 and AHA-1742A; Future
Domain TMC-1670, TMC-850M and MCS-600; IBM PS/2 Microchannel SCSI Host
Adapter (with cache); Ultrastor 24fa. Drives listed with * support
multimedia audio.
 
*CD-Technology CD Porta-Drive T-3301
*CD-Technology CD Porta-Drive T-3401
Chinon 431 [25]
*Chinon 535
*COMPAQ DualSpeed CD-ROM Drive
DEC RRD 42-DA
Denon DRD 253 [26]
Hitachi ® CDR-1750S
*Hitachi CDR-3750S
IBM 3501 [25]
*IBM Enhanced Internal CDROM II Drive 32G2958
*IBM Enhanced External CDROM II Drive 3510005
*IBM PS/2 CDROM II Drive
*NEC Intersect CDR-73M [27]
*NEC Intersect CDR-83M
*NEC Intersect CDR-74
*NEC Intersect CDR-84
*NEC Intersect CDR-74-1
Panasoni ® CR-501B [25]
Philips / Laser Magnetic Storage CM-215 [28]
*Pioneer ® DRM-600 [29]
Plextor DM-5021 [25] (same as Texel DM-5021)
*Plextor DM-5024 [30] (same as Texel DM-5024)
*Procom Technology MCD-DS
*Sony CDU-541
*Sony CDU-561
*Sony CDU-6211
*Sony CDU-7211
Texel DM-5021 [25] (same as Plextor DM-5021)
*Texel DM-5024 [30] (same as Plextor DM-5024)
Toshiba ® TXM-3201 [25]
*Toshiba TXM-3301
*Toshiba TXM-3401
 
Other CD-ROM Drives
===================
 
The following CD-ROM drives with proprietary interfaces have been
tested. Drives listed with * support multimedia audio.
 
++Creative Labs Sound Blaster Pro [TM]
++Panasonic CR-521
++Panasonic CR-561
*++Sony ® CDU 31a
 
SCSI Tape Drives
================
 
The following SCSI tape drives have been tested with the following
adapters using the Windows NT Backup utility: Adaptec AHA-1510, AHA-
1542C, AHA-1640 and AHA-1742A; Future Domain TMC-1670, TMC-850M and
MCS-600; IBM PS/2 Microchannel SCSI Host Adapter (with cache);
Ultrastor 24fa. Drives are listed under their appropriate Setup Tape
entry.
 
4 Millimeter DAT
----------------
 
    ArchiveST 2000DAT (4520NP, EAX4350) [31]
    ArchiveST 4000DAT (4324NP, 4352XP)
    Exabyte 4200 [32]
    Exabyte 4200c [33]
    Hewlett-Packard JetStor 2000
    Hewlett-Packard JetStor 5000
    Hewlett-Packard 35470a [31, 34]
    Hewlett-Packard 35480a
    Hewlett-Packard C1503a [31, 34]
    Hewlett-Packard C1504a
    Hewlett-Packard C2224c [31, 34]
    Hewlett-Packard C2225b
    ++IBM 2.0Gb 4mm Tape Drive Option
    Maynard Maynstream 1300DAT
    Maynard 2000 DAT
    Tecmar DataVault 2000
    Tecmar DataVault 4000
    WangDAT Model 1300XL
    WangDAT Model 3100
    WangDAT Model 3200
 
Archive ® 2150S, 2525S, 2750
------------------------------
 
    Archive 2150/2250 [35]
    Archive 2525
    Archive 2750
    Archive 2800
 
Exabyte 8200 Series (SCSI-1)
----------------------------
 
    Exabyte EXB-8200 [34, 35]
    Exabyte EXB-8200ST [34, 35]
    Exabyte EXB-8205 [32]
    Exabyte EXB-8205ST [32]
 
Exabyte 8500 Series (SCSI-2)
----------------------------
 
    Exabyte EXB-8500
    Exabyte EXB-8500ST
    Exabyte EXB-8500c [34]
    Exabyte EXB-8500cST [34]
    Exabyte EXB-8505
    Exabyte EXB-8505ST
    IBM 5.0Gb 8mm Tape Drive Option
    IBM 3445 Model 001 5.0Gb 8mm Tape Drive
 
Tandberg 3660, 3820, 4120, 4220
-------------------------------
 
    IBM 3450 1.2Gb Tape Drive Model 001
    Tandberg 3660
    Tandberg 3820
    Tandberg 4120
    Tandberg 4220
 
Wangtek 525, 250
----------------
 
    Tecmar QT-525ES
    Wangtek 5150ES
    Wangtek 5525ES
    Wangtek 51000ES
 
Technical Notes
---------------
 
Items listed with ++ are supported with device drivers available in the
Windows NT Driver Library.
 
 1 Refer to SETUP.TXT for information on configuring this
   machine/device before installation.
 2 Only the NCR 53c710 SCSI Host Adapter is supported in this machine.
 3 Contact the manufacturer for information on running Windows NT on
   this machine.
 4 Tested with firmware revisions 3.10 and 3.20.
 5 This adapter requires an active terminator for proper performance.
 6 This adapter must be configured for 5 MB/second asynchronous I/O to
   work with listed CD-ROM drives from NEC.
 7 This adapter must be configured for 5 MB/second asynchronous I/O to
   work with listed CD-ROM drives from Chinon, Hitachi and NEC.
 8 Tested with the Unisys PW2 Advantage 3256 (Flemington).
 9 Tested with the Unisys PW2 Advantage Plus MPE 4668.
10 Removable media drives are not supported with cache module
   installed.
11 CD-audio, tape drives and scanners are not supported on this
   controller.
12 To use this adapter, at least one device on the bus must provide
   termination power.
13 Refer to SETUP.TXT for information on configuring this adapter.
14 SCSI BIOS dated before 1991 requires PS/2 Reference Diskette
   version 1.21 or later.
15 This adapter cannot be used for CD Setup. To install Windows NT
   with this adapter, use the WINNT.EXE Setup method.
16 Scanners are not supported with this adapter.
17 Tested with COMPAQ Portable 486c.
18 Tested with NCR System 3000 Model 3350.
19 This adapter is currently supported in its ESC-1/ESC-2
   compatibility mode only.
20 This adapter is a RAID controller which supports hard drives only.
21 This adapter is only supported on IRQ-5.
22 This adapter is only supported for use with scanners and CD-ROM
   drives.
23 Tested with firmware revision 005.
24 Tested with firmware revision 008.
25 Audio is not supported on this drive.
26 This drive is not supported for use with the Adaptec AHA-1542c.
27 This drive requires double-termination when used with the Adaptec
   AHA-1742A.
28 This drive is not supported for use with the Future Domain TMC-850M
   and TMC-1670 adapters.
29 The Adaptec AHA-1640 and Ultrastor 24f support only a single disk
   when used with this drive. This drive is not supported for use with
   the Future Domain MCS-600 adapter.
30 Requires firmware revision 1.10C to function properly with Windows
   NT.
31 This drive is not supported with the Adaptec AHA-1640 adapter.
32 This drive is not supported with the IBM PS/2 Microchannel SCSI
   Host Adapter (with cache).
33 This drive is not supported with the Future Domain TMC-850M(ER).
34 This drive is not supported with the Adaptec AHA-1742A adapter.
35 This drive is not supported with the UltraStor 24fa adapter.
36 For use with floppy controllers. Separate interface controllers for
   these types of drives are not supported.
37 Requires that 512-byte sector-sized media be mounted during
   installation.
38 Tested with HP C2225B tape drive, HP C2229B disk drive and HP
   C2226A CD-ROM drive.
39 Supported in Sound Blaster 1.x compatibility mode.
40 Not supported in Sound Blaster 1.x compatibility mode.
41 Error control and flow control forced on.
42 Advanced features disabled.
43 Supported as a client modem only.
44 Flow control forced on.
45 Maximum DTE speed set to 2400.
46 Maximum DTE speed set to 9600.
47 Modem compression forced on.
48 In the UPS applet, check the box "Remote UPS Shutdown" and set it
   to high.
 
Additional reference words: prodnt 3.10 HCL
KBCategory: kbhw
KBSubCategory: nthw HCLIST
 
=============================================================================
 
Copyright Microsoft Corporation 1994.
