;
; Entries to be added to the RAS MODEM.INF file for
; ECCI modems.
;
;----------------------------------------
[ECCI Modan 14400]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

; speaker settings not applicable
;<speaker_on>=M1
;<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
;use both %C and appropriate S46 settings to work correctly
<compression_on>=%C3S46=138
<compression_off>=%C0S46=136
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RCV144DPL Rev <?><?>

COMMAND_INIT=AT&F&C1&D2&R1Q0V1E1X4 S0=0 S7=55 S2=128<cr>

;to get short responses
;COMMAND_INIT=ATW0S95=0<cr>
;to get long responses
COMMAND_INIT=ATW1S95=44<cr>

COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[ECCI Modan 28800]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

; speaker settings not applicable
;<speaker_on>=M1
;<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
;use both %C and appropriate S46 settings to work correctly
<compression_on>=%C3S46=138
<compression_off>=%C0S46=136
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RCV288DPL Rev <?><?>

COMMAND_INIT=AT&F&C1&D2&R1Q0V1E1X4 S0=0 S7=55 S2=128<cr>

;to get short responses
;COMMAND_INIT=ATW0S95=0<cr>
;to get long responses
COMMAND_INIT=ATW1S95=44<cr>

COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

