1
1

# The first line in this file must have only an ASCII digit string representing
# the MPCM minor number format version. The following formats are supported
# at this time:
#	0 - Version 1.0 -- old standard.
#	1 - Version 2.0 -- new version supporting 4 channels per LM.
# This file must exist in the /usr/etc/scom directory on the target machine.

# The second line in this file must have only an ASCII digit string representing
# the MPCM LM configuration format. This value has meaning only when using
# the MPCM minor number format version 2.0 or greater (first value >= 1).
# The following formats are supported
# at this time:
#	0 - old format with A and B channels configured only.
#	1 - new format supporting configuration of 4 channels per LM.
#
#
# This file must exist in the /usr/etc/scom directory on the target machine.
#
# !NOTE! For NT releases, leave the ^M after the numbers.
