;       
;       (c) Copyright Cabletron Systems Inc. 1992
;
;       Cabletron Systems Inc.
;       P.O. Box 5005
;       Rochester, NH 03867-5005
;
;       F3069 Micro Channel FDDI Adapter
;       Mon Nov 9, 1992
;        - 
;       Version 0.00.02
;       Norm Smith
;
AdapterId 0070h
AdapterName "Cabletron Systems Inc. F3069 FDDI Adapter"
NumBytes 4

NamedItem
       Prompt  "Chip Select for I/O Base Address"
       choice "Base address: 0300"
              pos[0]=000XXXXXb        io      0300h - 033Fh
       choice "Base address: 1300"
              pos[0]=001XXXXXb        io      1300h - 133Fh
       choice "Base address: 2300"
              pos[0]=010XXXXXb        io      2300h - 233Fh
       choice "Base address: 3300"
              pos[0]=011XXXXXb        io      3300h - 333Fh
       choice "Base address: 4300"
              pos[0]=100XXXXXb        io      4300h - 433Fh
       choice "Base address: 5300"
              pos[0]=101XXXXXb        io      5300h - 533Fh
       choice "Base address: 6300"
              pos[0]=110XXXXXb        io      6300h - 633Fh
       choice "Base address: 7300"
              pos[0]=111XXXXXb        io      7300h - 733Fh

Help                         
"This is the base address for the I/O section of
the F3069 FDDI adapter.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."


NamedItem
       Prompt  "Boot ROM Base Address"
       choice "Boot ROM not installed"
              pos[0]=XXX111XXb        
       choice "Base address: 0C8000"
              pos[0]=XXX000XXb        mem     0C8000h - 0CFFFFh
       choice "Base address: 0D0000"
              pos[0]=XXX010XXb        mem     0D0000h - 0D7FFFh
       choice "Base address: 0D8000"
              pos[0]=XXX100XXb        mem     0D8000h - 0DFFFFh
       choice "Base address: 0C0000"
              pos[0]=XXX110XXb        mem     0C0000h - 0C7FFFh

Help
"This is the address for the Boot ROM.  If there is
no ROM installed, selecting other than 'Not Installed'
will cause erratic system operation.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."



NamedItem
       Prompt "24 or 32 Bit Addressing"
       choice "24 Bit Address" pos[2]=XXXXXXX1b
       choice "32 Bit Address" pos[2]=XXXXXXX0b

Help
"When the F3069 FDDI Adapter is bus master, this bit
is used to tell it whether to use 24 or 32 bit
addressing.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."



NamedItem
       Prompt "Interrupt Level"
       choice "Level 3 "       pos[1]=000XXXXXb Int 3
       choice "Level 5 "       pos[1]=001XXXXXb Int 5
       choice "Level 7 "       pos[1]=010XXXXXb Int 7
       choice "Level 9 "       pos[1]=011XXXXXb Int 9
       choice "Level 10"       pos[1]=100XXXXXb Int 10
       choice "Level 11"       pos[1]=101XXXXXb Int 11
       choice "Level 12"       pos[1]=110XXXXXb Int 12
       choice "Level 14"       pos[1]=111XXXXXb Int 14

Help
"This is the selection for the Interrupt Level that
the F3069 FDDI Adapter will use.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."



NamedItem
       Prompt  "Arbitration Level"
       choice "Arbitration Level 8 "   pos[1]=XXXX1000b arb 8
       choice "Arbitration Level 9 "   pos[1]=XXXX1001b arb 9
       choice "Arbitration Level 10"   pos[1]=XXXX1010b arb 10
       choice "Arbitration Level 11"   pos[1]=XXXX1011b arb 11
       choice "Arbitration Level 12"   pos[1]=XXXX1100b arb 12
       choice "Arbitration Level 13"   pos[1]=XXXX1101b arb 13
       choice "Arbitration Level 14"   pos[1]=XXXX1110b arb 14
       choice "Arbitration Level 0 "   pos[1]=XXXX0000b arb 0
       choice "Arbitration Level 1 "   pos[1]=XXXX0001b arb 1
       choice "Arbitration Level 2 "   pos[1]=XXXX0010b arb 2
       choice "Arbitration Level 3 "   pos[1]=XXXX0011b arb 3
       choice "Arbitration Level 4 "   pos[1]=XXXX0100b arb 4
       choice "Arbitration Level 5 "   pos[1]=XXXX0101b arb 5
       choice "Arbitration Level 6 "   pos[1]=XXXX0110b arb 6
       choice "Arbitration Level 7 "   pos[1]=XXXX0111b arb 7

Help
"This is the priority level that the F3069 FDDI
adapter uses when it wants to be Bus Master.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."


NamedItem
       Prompt  "Bus Master Fairness"
       choice "Enabled "       pos[1]=XXX1XXXXb
       choice "Disabled"       pos[1]=XXX0XXXXb

Help
"This tells the bus arbitration circuitry to use the
fairness algorithm when requesting the use of the bus.
Use the F5=Previous and the F6=Next keys to change
this assignment in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk
and must be changed to use the adapter."

