## Configuring SunMC

1. Configure the Storage Automated Diagnostic Environment to send a topology to the SunMC server host.
2. Snap the topology using the Storage Automated Diagnostic Environment. Refer to the Create a Topology Snapshot section of the online help.
3. Load the SunMC `rasagent` module onto the SunMC server host.
4. Configure the `rasagent` module to point to the Storage Automated Diagnostic Environment.
5. Configure the Storage Automated Diagnostic Environment SunMC Provider to point to the SunMC server host.

Note -

If they are already running, stop the SunMC agents, and repeat the steps above.

Caution -

Do not configure the SunMC software, or any other software, directly onto the Storage Service Processor. If, for some reason, software was directly installed onto the Storage Service Processor, uninstall it, as it is not part of the SP image.
The Service Processor does not use the SunMC provider. Instead, install the SUNWstade package on a non-Service Processor host that has out-of-band access to Sun.