## SunMC Provider

The SunMC Provider enables the Storage Automated Diagnostic Environment to send actionable events and monitoring topologies to the SunMC Console, which displays the alarms and alert text. SunMC information is similar to and compatible with Sun Remote Services (SRS). SunMC can send information to SRS, in which case the SRS Provider need not be activated in the Storage Automated Diagnostic Environment.

Once activated, the SunMC module receives information about monitored devices and displays alarms in the SunMC console.

All available instrumentation, events, and topology information is sent to the Network Storage Command Center (NSCC). This information is monitored by Sun Service personnel and is used to improve products and service.

Note -

Each SunMC agent can handle one Storage Automated Diagnostic Environment master. The SunMC console will aggregate events if your site has multiple masters.