## `6120ofdg` Test Options

The `6120ofdg`(1M) test runs the internal diagnostics of the Sun StorEdge 6120 array.

Before you run the 6120ofdg(1M) test, you must first do the following:

- Run the Storage Automated Diagnostic Environment manually by following the procedures explained in "Running the ras_install Script".
- Generate a report for the device against which you are running the test (for example, Sun StorEdge 6120 arrays).

If the number of existing volumes do not match, an error message is displayed.

Note -

This test requires the user to enter the user ID and password options for the Sun StorEdge 6120 array that is being tested. Use the Update Device section of "Maintaining Devices" to add an optional 6120 password.

Option | Description
--- | ---
Syslog Dump | Enable will dump all syslog entries that have been added, while the test is running, to the screen. ofdg will dump only OFDG lines, added to the syslog, to the screen. The default is Disable.
Fast_Test | Fast_Test performs a fast Go/No Go test of the selected enclosure and loop. It does not attempt to detect bad FRUs. The default is Enable.
Health_Check | Health_Check runs Fast_Test multiple times, one time for each loop per unit. The default is Disable.
Fast_Find | Fast_Find can be used to detect bad loop cards, interconnect cables, and controllers. Fast_Find does not try to isolate down to a single disk port. Run Fast_Find before Find to eliminate loop cards, interconnect cables, and controllers as bad FRUs before the midplane or disks are suspended (which are checked using Find). The default is Disable.
Find | Find performs an extensive Go/No Go test. If loop failures are detected, it automatically initiates the full-loop-fault-isolation diagnostic. The loop fault diagnostic has the capability to detect and isolate a single disk port but is very time-consuming. The default is Disable.
Loop | Loop specifies which loop to test. All tests both loops. The default is All.
Password | The Sun StorEdge 6120 array telnet password enables the Storage Automated Diagnostic Environment to log into the Sun StorEdge 6120 array device. The password is required.

Note -

You cannot change an existing Sun StorEdge 6120 array password. If no password exists, however, you can add a password using the information found in "Sun StorEdge 6120 Array Passwords."

### CLI Help Man Page

`6120ofdg`.1m