## Running Diagnostic Tests from the GUI

If you run the diagnostic test using the Storage Automated Diagnostic Environment, you can easily access test configuration, control, and results, using the buttons in the dialog boxes. In addition, you can use the GUI to perform the following tasks.

- Enables you to access diagnostic tests from a topology view.
- Enables you to access diagnostic tests from a list.
- Enables you to adjust the default settings for selected diagnostic tests.
- Enables you to review, delete, or archive diagnostic tests.
- Enables you to review the results of old tests.

The diagnostic tests are designed to test the target FRU and to operate on an in-band or out-of-band data path. The Storage Automated Diagnostic Environment scheduler dispatches the test to be run on the appropriate server (host).