## Accessing the Monitor Topology Page

1. Click the Monitor link on the Storage Automated Diagnostic Environment main window.
2. Click the Monitor Topology link.

A blank Topology window is displayed.

Note -

To view a topology, you must first do the following:

3. Execute the command `/opt/SUNWstade/sysbin/config_solution` to create the topology, find the devices, and run the agents.
4. After device discovery, create a Topology snapshot.