## Testing from Topology

1. Click the Test from Topology link.

The Test from Topology window is displayed.

2. Using the right mouse button, select the device.

A list of test options appears.

3. With the left mouse button, select the test you want to run on the device.

The applicable test is displayed in the right pane.

4. Select the Clear link in the Topology view to remove all the green alert icons from the topology. The red and yellow alert icons remain in the topology until all faults have been corrected.

Note -

If a red "mpxio" label is displayed in the Topology, a Sun StorEdge Traffic Manager failover has been discovered on this path.
If a green "mpxio" label is displayed in the Topology, a Sun StorEdge Traffic Manager failover has occurred on this path, but was later corrected.

While a test is running, the Test Manager pop-up window appears and reports the status of the test. See "Test Manager" for more information.

After the test has completed its run, an email message is sent to the specified email recipient.