## Using Test Manager

The Storage Automated Diagnostic Environment's integration with diagnostic tests implements Test Manager to track and control the progress of the user-selected tests. The Test Output view enables you to view test output for active and completed tests in the Test Monitor view.

The Storage Automated Diagnostic Environment runs the device tests in a distributed manner. The master calls the proper host to begin tests (device edition only).

Note -

To sort in Test Manager, click on the header for any column and the list sorts the entries in that column. A plus ("+") indicator signifies that this is the current sort.

For test processes, the status (displayed in the Test Manager Status column) can be one of the following:

- Running-User intervention is required for the test to continue. User intervention may involve answering a question or replacing the cables or the gigabit interface converters (GBICs).
- Done OK-The test ran successfully with no errors.
- Done Error-The test failed and no longer continues to run.
- Done Aborted-The user manually stopped the test before it had finished running.

Note -

There is a system time-out associated with the Waiting state. If you want to change the default settings for scheduled time-outs, see Changing System Time Out Settings.