## Sun StorEdge 6120 Array Passwords

The `6120volverify` test requires a user ID and password for the Sun StorEdge 6120 array that is being tested.

The Storage Automated Diagnostic Environment test will use the user id and password that were set up using the steps in "To Add Information About a Device." If no password exists for the Sun StorEdge 6120 array, you can add a password using "To Update a Device Manually."

Option | Description
--- | ---
VolumeName | VolumeName is the name of the volume to verify. Note that the volume name is a name internal to the array and is not seen by the host.
Fix_Errors | The Fix_Errors option corrects parity errors on RAID 5 volumes and corrects mirrored data errors on RAID 1 volumes. If Fix_Errors is not specified, then `6120volverify` will report errors but not correct them. If the Fix_Errors option is specified and an error is detected, the 6120volverify command will regenerate parity from the existing data on the volume.
Rate | Rate refers to the speed at which the `6120volverify` is run. The verification rate is n, where n equals any number from 1 to 16. The default rate is 1, which has the minimum performance impact on the data host. 16 has the highest performance impact on the data host.
Password | The Sun StorEdge 6120 array telnet password enables the Storage Automated Diagnostic Environment to log into the Sun StorEdge 6120 array device. The password is required.
Note: You cannot change an existing Sun StorEdge 6120 array password. If no password exists, however, you can add a password using the information found in "Sun StorEdge 6120 Array Passwords."

### CLI Help Man Page

- `volverify.1m`