Volume Verify |

This option will execute volume verify continuously on all arrays at the selected rate. Volumes are verified one at a time on a rotational basis. Events are generated when this operation fails.
This option applies only to Sun T3, Sun 6020 and Sun 6120 arrays.
Volume verify can also be turned on or off on a device by device basis in General Maintenance -> Maintain Device. The 'Default Array Password' is used when there is no password entered in Administration -> General Maintenance -> Maintain Device for a specific array.
This option is not considered a diagnostic and does not impact monitoring coverage. Green and yellow disk led will be lit when this oparation is running.
Warning: Using the 'fix' option on vol verify may fix parity on bad blocks. This can sometimes hide corrupted data blocks.

Use 'Kill Verify' to kill 'vol verify' on the arrays that are monitored and where vol verify was started by Storage A.D.E.

The 'Device Summary' displays each monitored array with the following fields:

- Verify: Is the continuous 'vol-verify' option turned-on for this device.
- Last Volume: The last or current volume being verified.
- Start: Start date of the last 'vol-verify'.
- Status: The progress of vol-verify or the word 'Start' or 'KILL'.