## Configuring the SunMC Server Host

1. Open the SunMC console.
2. Click the SunMC Server Host icon.
3. Select the Modules tab.
4. Select `rasagent` from the Available Modules list.
5. Click Load.
6. Type the SunMC Server IP address in the `rasagent` Provider IP text box.
7. Check Remove Saved Topology.

This step is important. If you do not check it, SunMC will report on the previously-saved topology.

8. Click OK.
9. Click the Module Browser tab.
10. Click the Hardware icon.
11. Check to make sure the `rasagent` icon is displayed in the Hardware subtree.
12. Double-click the `rasagent` icon to display the subtree folders of components.