## Adding Devices

1. From the Administration--> General Maintenance window, click Add Devices.
2. Type the required input for each device is as follows:

Note -

The Sun StorEdge 3120 and 3310-D SCSI (JBOD) Arrays must be added to the Storage Automated Diagnostic Environment using the In-Band discovery function.

### Sun StorEdge 3310, 3510, and 3511 Fibre Channel (RAID) Arrays

1. Click Sun 3310/3510/3511.
2. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
3. Select the Storage Automated Diagnostic Environment host that will perform the actual monitoring of the device.
4. enter the IP Name or IP Address of the array.
5. Click Add.

### Sun SAM-QFS

Adding SAM-QFS that is installed on a networked host allows the Storage Automated Diagnostic Environment to monitor SNMP traps from SAM-QFS about tape drives and library hardware in the SAM-QFS configuration.

SNMP traps are displayed in the Storage Automated Diagnostic Environment as events and alarms from the SAM-QFS host.

1. Specify the Network Information Services (NIS) name of the host on which SAM-QFS is running.
2. Select the host on which SAM-QFS is running. Options include Local, and all hosts known to the Storage Automated Diagnostic Environment.
3. Specify the IP Name or IP Address of the host on which SAM-QFS is running.
4. Click Add.

Sun SAM-QFS is added as a device from which the Storage Automated Diagnostic Environment receives SNMP traps.

Note -

SAM-QFS also must be configured to send SNMP traps to the Storage Automated Diagnostic Environment. Refer to the Sun StorEdge QFS and Sun StorEdge SAM-FS Installation and Configuration Guide for more information.

### Sun StorEdge A3500FC Array

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Enter the serial number for the device.
3. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.

### Sun StorEdge A5000 array

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.

### Brocade Silkworm switches

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
3. Type the optional telnet password, which enables the Storage Automated Diagnostic Environment to log into the Brocade switch.
4. Type the IP address that identifies the host to the network.

### Sun StorEdge D2 array

1. Type the device path with which the Storage Automated Diagnostic Environment will access the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
3. Type the serial number of the Sun StorEdge D2 array, which will be used to identify the device to the host.

### Internal FC Disk

- Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.

### Inrange FC Switch

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
3. Type the IP address that identifies the switch to the network.

The host that will be monitoring this device must have SNMP access enabled from the Inrange management GUI.

### Sun StorEdge Network FC Switch-8 and Switch-16 Switches

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
3. Type the optional admin telnet password, which enables the Storage Automated Diagnostic Environment to log into the Sun switch.
4. Type the IP address that identifies the host to the network.

### Sun StorEdge 6120 Array

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Type the optional telnet password, which enables the Storage Automated Diagnostic Environment to log into the Sun StorEdge 6120 array device. Note that the user is not authorized to change an existing Sun StorEdge 6120 array password.
3. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
4. Type the IP address that identifies the host to the network.

### FC Tape

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.

### Sun Fire V880 FC-AL Disk

1. Type the device name the Storage Automated Diagnostic Environment will use to identify the device.
2. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.

### Virtualization Engine

1. Select the Storage Automated Diagnostic Environment's primary host that will perform the actual monitoring of the device.
2. Enable the Turn Monitoring On button.

1. After you have finished entering device information, click Add.
2. To return to the Add Devices screen, click Back.

### Related Topics

- Maintain Devices