## System Timeouts Page

Setting | Definition
Ping | The timeout used to perform a ping. The default is 10 seconds.
Email | The timeout used when sending email messages. The default is 30 seconds.
Sun Storage Arrays (http tokens) | The timeout used when extracting token information from a Sun StorEdge 6120 array. The default is 60 seconds.
SNMP access | The timeout used to query switches that support Simple Network Management Protocol (SNMP). The default is 60 seconds.
luxadm (Sun A5000) | The timeout for the Sun StorEdge A5x00 array luxadm. The default is 600 seconds.
RM6 (Sun A3500FC) | The timeout (in seconds) for the Sun StorEdge A3500FC Raid Manager interface (RM6). Users change the timeout if RM6 is slow to respond during monitoring. The default is 200 seconds.
Discman (Discovery) | Discovery timeout. The default is 1200 seconds.
slicd (VE) | Virtualization Engine timeout. The default is 180 seconds.
sccli | No default; user input is required.