Patch-ID# 117371-05
Keywords: sun fire 15k hpost redx libxcpost.so
Synopsis: SMS 1.4.1: hpost redx libxcpost.so patch
Date: Oct/21/2004


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.4.1

Xref: 

Topic: SMS 1.4.1:

Relevant Architectures: sparc

BugId's fixed with this patch: 4774140 4838858 4934573 4943893 4971389 4975645 5019759 5023600 5026899 5030572 5030612 5030965 5033832 5042013 5047640 5049383 5055895 5064369 5064481 5066219 5070022 5074115 5081526 5088108 5096410 5101378 5102667 5102841 5103413 5103433

Changes incorporated in this version: 5081526 5088108 5096410 5101378 5102667 5102841 5103413 5103433

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.4.1/bin/hpost
/opt/SUNWSMS/SMS1.4.1/bin/redx
/opt/SUNWSMS/SMS1.4.1/lib/libxcpost.so

Problem Description:

5081526 wfail misdiagnoses memory MTag UE/NE DStop
5088108 wfail should not ignore DCDS DPE for US4 procs 3.1 and later
5096410 Don't use unreliable DX errors on Jag brds for diagnosis
5101378 Redx display for xmits chip should include a revision number field
5102667 Confusing message from redx on non-SC platform
5102841 Add support for lpost version 5.17.2, and support with up-rev warning for 5.18.0
5103413 A failed I/O board BBC should cause the board to be crunched
5103433 I/O cage POST names Service FRU for RStop in domain
 
(from 117371-04)
 
4774140 seeprom on hPCI+ not in dump
4838858 redx use of DX pause timeout
4934573 SMS redx/post/etc should handle compressed dump files
5047640 post on xmits 2.1 does not recognize the CID at high verbosity
5049383 wfail misdiagnoses a datapath UE fault on the EXB.
5055895 Hpost should support lpost 5.17.1 without warning message
5064369 wfail FRU misidentification of a clock failure on CSB
5064481 hpost -H of MaxCPU IOxx fails if SBxx in target domain, vice versa
5066219 Irrelevant processor error printed by wfail.
5070022 Excessive xcstate files created during hpost -Q
5074115 Change control method for engineering .postrc commands
 
(from 117371-03)
 
5026899 SMS POST support for 1200 MHz USIV processors
 
(from 117371-02)
 
4943893 dstop during POST - AXQ and SDI are inconsistant
4971389 Jaguar SB indicated as primary service FRU during DR to a MCPU domain
4975645 Allow MaxCPU in split expander with AXQ 6.3
5023600 wfail should recognize EXBs reset during operation
5030572 Skip hsPCI+ workaround for AXQ 6.3
5030612 force_axq_xmits_throttle_vector doesn't work if only slot 0 present.
5030965 Accept AXQ 6.3 without warning
5042013 starcat post needs to support xmits 2.1 with out warning message
 
(from 117371-01)
 
5019759 Add retries for XIRs used for I/O test cage.
5033832 Add retries for XIRs during POST

Patch Installation Instructions:
--------------------------------
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Required patches:
        Solaris patch 113027-04 if running Solaris 9
        Solaris patch 117002-02 if running Solaris 8
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).

README -- Last modified date:  Thursday, October 21, 2004

