Patch-ID# 142700-02

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************
For further information on patching best practices and resources, please
see the Big Admin Patching Center, http://www.sun.com/bigadmin/patches/ 
***********************************************************************

Keywords: sun fire v210/v240 netra 210/240 obp rohs wanboot panther
Synopsis: Hardware/PROM: Sun Fire V210/V240 Netra 210/240 Flash PROM Update
Date: Feb/09/2010


Install Requirements: None                      
                      
Solaris Release: 8 9 10

SunOS Release: 5.8 5.9 5.10

Unbundled Product: Hardware/PROM

Unbundled Release: OBP 4.30.4.a, POST 4.30.4.a, OBDIAG 4.30.4.a

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4794955 4854322 4946025 5052695 5076888 5079065 5079227 6181985 6183557 6230349 6230541 6244643 6256046 6313800 6322957 6332576 6333076 6338777 6345852 6346530 6346885 6347315 6347502 6347549 6360432 6361002 6361535 6361563 6364139 6366588 6368614 6368716 6370015 6370405 6370408 6372458 6372564 6374738 6375003 6375990 6376524 6376657 6377038 6377208 6377849 6379703 6379876 6379878 6379979 6380442 6380622 6380975 6381064 6381084 6381105 6381115 6381125 6381242 6381271 6381272 6381274 6381277 6381279 6381281 6381283 6381385 6381818 6382974 6383237 6383658 6384335 6384845 6385582 6386216 6386341 6387399 6388093 6388582 6388673 6388925 6389161 6389988 6390526 6390564 6391361 6391455 6392539 6392742 6392744 6392749 6392873 6393492 6393665 6393953 6393958 6394040 6395015 6396318 6396464 6396519 6396528 6396533 6396540 6396546 6397170 6397497 6397564 6399215 6399627 6400117 6400192 6400408 6401634 6401719 6402905 6402909 6403073 6404798 6406061 6406091 6406142 6406195 6406577 6407069 6407889 6409416 6411051 6411069 6411912 6412462 6412474 6412550 6412889 6413467 6413698 6414799 6414995 6415442 6415545 6416036 6416142 6416169 6416658 6416671 6417885 6418642 6418658 6419216 6420097 6420137 6420147 6420194 6420241 6420886 6421308 6421344 6421833 6421866 6421884 6421977 6422104 6422818 6422909 6423038 6423090 6423131 6423137 6423761 6423788 6423795 6423803 6424432 6424812 6425918 6426346 6427093 6427102 6428852 6428946 6429329 6430079 6430086 6430219 6430500 6430572 6431870 6432504 6433152 6436266 6436300 6436354 6436371 6438159 6438649 6438710 6441770 6441889 6442350 6443014 6444152 6445593 6447320 6447326 6447642 6447749 6447763 6447810 6447815 6447818 6447820 6447821 6447824 6447852 6448085 6448548 6449538 6449659 6450457 6450624 6451155 6451159 6451168 6451721 6451762 6451938 6452183 6452223 6452237 6452256 6454051 6455202 6456539 6456885 6456952 6457354 6458997 6459524 6459543 6459548 6459574 6460910 6460934 6463668 6464267 6465220 6465254 6466207 6466624 6466637 6466655 6466679 6466695 6467470 6468284 6468359 6469964 6470467 6470510 6470888 6471999 6472605 6474333 6474932 6478131 6478437 6478646 6480310 6480389 6481526 6481980 6482540 6484677 6484976 6485717 6485941 6487271 6487277 6487287 6487292 6487301 6487332 6487343 6487348 6487438 6487708 6488846 6488855 6490115 6491132 6494774 6494859 6495912 6498373 6498780 6500285 6500287 6500325 6503261 6504355 6504375 6505653 6505657 6505760 6506771 6508437 6508449 6508466 6508474 6508906 6510676 6510693 6510722 6511659 6511901 6512278 6512280 6512314 6512782 6512892 6513595 6515491 6516619 6517108 6517207 6518846 6518865 6518879 6518883 6519920 6519943 6520058 6520718 6521186 6521198 6521605 6521645 6523024 6523823 6524613 6525090 6525913 6526107 6526454 6526699 6526861 6526870 6527778 6528635 6528667 6529207 6529467 6529504 6529934 6532334 6534028 6534031 6535840 6537035 6538367 6539675 6540632 6543430 6543748 6543749 6545197 6545200 6545566 6546593 6547428 6548060 6549753 6550351 6550398 6550717 6550743 6550784 6551724 6553004 6554358 6557874 6558342 6559998 6561842 6561957 6566732 6569526 6570315 6570779 6572821 6573367 6573618 6574092 6574105 6575253 6576406 6579294 6580761 6581085 6581490 6581660 6581794 6583392 6585340 6586400 6587533 6588214 6589154 6589571 6590254 6590384 6590912 6592973 6592986 6593097 6593547 6594395 6594929 6595500 6596546 6596594 6598829 6600945 6601551 6601822 6604051 6604845 6605782 6606197 6608466 6609024 6609130 6611798 6612022 6612178 6616363 6617193 6621175 6622444 6622775 6623111 6623916 6626045 6628699 6629201 6631330 6631946 6633009 6634169 6634974 6634977 6634980 6636978 6638534 6638972 6640485 6644446 6646461 6646532 6646995 6647462 6647984 6650227 6650783 6651513 6652016 6652046 6654860 6654865 6655556 6656072 6657721 6660206 6661787 6662162 6664365 6665538 6666961 6669255 6669488 6670340 6671070 6672367 6674578 6675519 6675677 6675793 6676561 6677840 6678885 6678924 6681061 6682845 6683328 6684123 6684913 6686172 6687097 6688605 6689868 6690618 6690844 6690952 6690978 6693035 6693734 6693906 6694304 6694387 6694497 6697436 6698815 6704491 6705064 6705118 6706303 6706473 6708044 6708234 6708608 6710322 6712358 6712366 6712395 6712683 6713501 6716256 6717373 6719274 6719316 6719407 6720177 6720401 6720575 6721020 6721347 6724265 6725256 6725717 6726148 6728454 6729529 6730281 6730282 6730722 6731112 6732222 6732265 6734408 6735506 6736372 6737081 6737476 6737895 6738373 6739392 6740949 6743825 6747230 6747621 6750734 6751051 6753562 6754453 6755425 6755818 6756295 6760186 6762055 6766240 6770610 6772664 6774655 6777379 6780222 6782337 6787965 6790291 6791196 6791232 6795793 6797789 6802075 6803726 6804349 6807094 6807927 6808167 6809434 6810138 6810143 6812437 6813603 6813715 6816141 6819881 6821770 6825151 6830927 6835857 6835860 6836888 6836962 6839482 6842259 6842274 6855840 6855850 6855865 6858855 6859020 6859443 6860195 6862099 6862229 6866918 6867960 6868081 6869577 6890136

Changes incorporated in this version: 6890136 6869577 6868081 6867960 6866918 6862229 6862099 6860195 6859443 6859020 6858855 6855865 6855850 6855840 6842274 6842259 6839482 6835860 6835857 6821770 6819881 6797789 6738373 6725717 6588214 6580761

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

flash-update-SunFire240
unix.flash-update.SunFire240.sh

Problem Description:

6890136 OBP 4.30.3.b causes ERROR: /pci@1d,700000/pci@1/<Unnamed>: Last Trap: Data Access Error
6869577 Insufficient memory allocated to the resolution buffer in the ast fcode.
6868081 Probe for TPM support in OpenBoot
6867960 Chalupa: POST Fails with ERROR: TEST = Slave Spin
6866918 Memory leak in SAS/SATA test 
6862229 speedup of mailbox test
6862099 Multiple resets observed
6860195 Add support to dump PLX FW from DEMON menu
6859443 POST sometimes picks the wrong channel in single channel mode
6859020 POST register assumption
6858855 Integrate AST2100 Fcode into source tree
6855865 Need to increase hotplug-memsize and hotplug-mem64size
6855850 Need to extend the Maximum PCI probe depth
6855840 Add the PCIe Root Port support for RCs containing RPs.
6842274 Speed up of L2 caches tests
6842259 Some of the internal L2 arrays are not being fully tested
6835860 POST timed out sometimes occurs
6821770 POST error occured on Neptune XAUI 10G Loopback Test
6797789 Confusing error messages when using PCIe cards with 64 bit prefetchable BAR
6738373 Correct Cheetah+ erratum 34 DTLB issue in Starcat OBP
6580761 OBP MMU miss handlers not correct for sun4v spec
 
(From 142700-01)
 
6839482 Need to remove clock-divisors from v445
6836962 Various errors reported during Tenaya P1.0 POST HDD testing, thought to be related to FMODs
6836888 Bootblock code in Solaris 10 Update 5 or earlier is incompatible with OpenBoot 4.30 or later
6835857 chip reset error occurs when OS boots
6830927 Some healthy components was disabled by a faulted DIMM
6825151 OBP console chars are dropped/scrambled with USB keyboard
6819881 Didn't receive RTR pkt! when powercycling huron and maramba systems
6816141 virtual storage devices are not getting created under OBP
6813715 POST Niu and Neptune Code Merge
6813603 POST thread bottleneck
6812437 DEMON selectable Systest BusFS causing NoData UEs
6810143 FMOD failures in POST SAS/SATA device test
6810138 Tenaya POST Support
6809434 OBP handles all resumable errors as request to shutdown
6808167 DEMON selectable Systest General test subtest conflict
6807927 VF System keeps power cycles and can't go to obp after POST test done
6807094 Congo:Need OBP changes for Firmware Progress State Sensor
6804349 DVD will not boot -- OBP fix missing to compliment CR 4976792 (READ RETRY)
6803726 Tenaya system (more than 1) hits fbr errors during Enhanced Memory testing
6802075 POST ops1 failed "FATAL ERROR 3", "Unexpected Trap" on N2 systems
6795793 POST look for display device on T6320
6791232 Monza: Need OBP changes for Firmware Progress Sensor
6791196 POST fails NIU Link Check Test w/ P1 Copper XAUI
6790291 Glendale/Scottsdale need to support REM-less operation
6787965 At post sequence, a CPU core was disabled by mistake, when a faulted DIMM was installed
6782337 POST disk test fails on phy7
6780222 The neptune fcode driver would break if bufsz0 were not set to 2K
6777379 Post support for T6320 G2
6774655 POST loops with "ERROR: No good memory bank/channel left in system" 
6772664 WARNING: /pci@7c0/pci@0/pci@1/pci@0/isa@2: Could not open asr package
6770610 Node Reconfig 2P with CPM1 and CMP3 ERROR: POST timed out. Not all system components tested.
6766240 DVD boot read failures from obp prompt (intermittent DVD DRIVE MISIDENTIFIED may be seen)
6762055 Booting from SATA DVD drives under LSI1068 fails
6760186 queue_tests_timed() function fails to complete under some conditions
6756295 Add support to test serial port from DEMON menu
6755818 Corruption of "my-self" causing missing "idprom" property in root node
6755425 More POST threads starting than expected
6754453 Maramba POST intermittently fails during the 100 power cycle with an LDOM created primary domain.
6753562 Failures of a secondary CMP master are not handled properly
6751051 POST reports hundreds of free resource timeouts
6750734 continuous output of "ERROR: Failed to send a fma event(rc=11)" during POST
6747621 RN50 fcode needs to support new memory
6747230 "1:4:0>ERROR: TEST = PIU intx interrupt test" is output during POST
6743825 POST menu IO-Bridge unit dump causes a crash
6740949 POST Block Mem Schmoo Test is N1 only
6739392 reset host causes POST to fail GBE tests
6737895 Some non-critical Neptune/NIU FCode clean up
6737476 OpenBoot disk label package fixes are mising from the large disk support changes
6737081 POST fails PIU PCI id test with ARTM
6736372 DVD boot error from IOU#2 or IOU#6 on DC machines generates wrong error log
6735506 POST is mis-handling a FBR error, if the FBR occurs too early in POST
6734408 Support change from remote-keyboard to rkeyboard in OBP
6732265 POST failures
6732222 nodefault-bytes is not persistent
6731112 Default case in init-xmac-xif sets mii-gmii-mode incorrectly 
6730722 LDOM Device RESET Control reg. is programmed with Maramba value in Scottsdale.
6730282 link up status message includes confusing "duplex = 0"
6730281 netboot via Maramba's Neptune port2 or 3 fails if a copper XAUI is plugged in
6729529 Product definition cleanup
6728454 remove support for N2 erratum 106
6726148 Power-cycling approx. 10 times causes disk devices to disappear.
6725717 V480 onboard CE failed OBDiag test intermittently
6725256 Miscellaneous fixes for OPL platforms
6724265 Initial PUTBACK of Scottsdale Blade to 4.28 and 4.x Gate
6721347 POST fails when X4447A-Z card present in slot PCIE3 or slot PCIE7
6721020 OpenBoot should handle "shutdown" request from Hypervisor
6720575 Add OBP support for Scottsdale Platform
6720401 POST should not fail the GBE device unless it is absolutely certain that the GBE is at fault.
6720177 POST fails with CMP0 missing on T5440
6719407 'Device:' is output 5 times after reset-all on OBP
6719316 USB Failure in POST indicts wrong device
6719274 Thrasher does not work on VF platforms
6717373 cpu-table should be clean before use
6716256 Thunder needs to pick updated OBP which has Scottdale fixes
6713501 Improve PCIE test and scan from post menus.
6712683 POST mistake the slot of the faulted DIMM
6712395 POST times out with 8GB FBDIMMs
6712366 Monitor preferred resolution does not work
6712358 POST print function confusion
6710322 Turgo POST fails when T1 PCI-X card is pluged in
6708608 master cpu timeout occuring on T5140/T5240
6708234 Glendale - watch-net-all terminates and jump by itself to OK when is looking at /niu@80/network@0
6708044 ipmi driver regression: broken on s10u3
6706473 post fails with 3-way config
6706303 post interrupt test fails on n1 platforms
6705118 Intermittent XAUI Lane Synchronization Failure at Flex.
6705064 POST, block memory test fails if thread 0 is asr disabled
6704491 OBP doesn't display all disabled devices
6698815 POST interrupt test updates
6697436 1G won't work if on Goa if a Goa in slot 1 is not inserted
6694497 POST incorrectly reports timeouts
6694387 OBP will try to run 10G copper at 1G
6694304 DMA function fails
6693906 probe-scsi-all generates Fast Data Access MMU Miss
6693734 Platforms that support MEM64 and PCI hotplug are using invalid memory sizes
6693035 Thunder POST still refers to non existent XAUI ports
6690978 Incorrect diagnosis of a memory UE
6690952 POST code implementation of Node reconfigure for T5440
6690844 Confusing PCIID test error messages
6690618 niu reset from guest doesn't properly prepare niu for 10g mode after running in 1g mode
6689868 With FW 7.1.3_build_02 "boot net - install" doesn't work
6688605 flx22610: Jade host hangs on a reboot with message ERROR: motherboard SEEPROM access failed
6687097 virtual-console device always returns NUL the very first character
6686172 TPM code incorrectly included in Congo POST makefile
6684913 Optimise enhanced POST Systest tests for N2 products
6684123 On OPL OBP can cause OBP to Display incorrect information
6683328 failure of some io devices disabled incorrectly
6682845 2 Unexpected trap37 when running memory screen
6681061 POST support for Thunder platform
6678924 Link width issue with plx version BC chip on pelton 
6678885 Link width issue with plx version BC chip on pelton
6677840 Enhanced POST memory tests on VF platforms should test local memory only
6676561 Changing NVRAM parameter at OS level causes panic : BAD TRAP: type=31
6675793 post hangs if diag verbosity=debug
6675677 POST membist test fails when CH0/D0 is disabled on a branch
6675519 Problem with LSB Degradation
6674578 Sparse CPU support for cpu-struct table
6672367 If a cmp has missing threads/cores in N1, then post will not test some regions of memory
6671070 POST diagnoses to a wrong dimm if a faulty dimm is in either D2 or D3 slots
6670340 Optimise enhanced POST memory tests for N2 products
6669488 POST times out with verbosity min
6669255 Domains fail to boot from the right devalias name
6666961 max level POST on Batoka with memory CE's gets unexpected trap to address 0
6665538 Ikkaku platform support
6664365 flx20948: CP2500 boot-device can be corrupted with a bad read from the AC
6662162 watch-net-all not testing interfaces
6661787 POST support for Batoka
6660206 Huron POST spelling error: "Lopback" missing an "o". eg:"ERROR: TEST = BCM8704 Internal Lopback".
6657721 POST should offline the failing DIMM module in the event of a CE.
6656072 post cpu tests failures, hardware under test is wrong field may state/fail wrong core
6655556 Updated P3 congo/post POST Support for Congo
6654865 OBP development for xaui copper
6654860 POST code setup for xaui copper
6652046 XAUI Conflicting error message
6652016 Sun Blade T6320 has no XAUI
6651513 version negotiation in obp's vnet/vdisk doesn't adhere to the protocol
6650783 PCI Probe error messages could cause problems
6650227 bootmode reset_nvram fails to reset obp to defaults
6647984 Thunder platform support in OBP.
6647462 Problem with T2000 SysFW 6.5.5, won't see DVD rom device after upgrade
6646995 POST output does not appear to be correct - POST is not correctly using SC's diag_<var> values
6646532 OBP providing incorrect compatible property at CPU node
6646461 OPL OBP Update copyright dates to reflect 2008
6644446 POST does not offline by thread when failing tests
6640485 post for maramba needs to be in 4x release gate
6638972 wanboot very slow on maramba
6638534 Maramba 2U with memory config. 24G and 48G on the mezzanine riser does not boot up the server.
6636978 setting input/output device via ok prompt to keyboard/screen results in ERROR: message
6634980 Possible Data corruption when using NVRAMRC kill or yank
6634977 POST run in max mode fails with PLX 8112
6634974 Incorrect Error reported on nvramrc CRC Error
6634169 flx22265: JLL13: no power-off on hotswap causes mcnet to fail to come up on Jade satellites
6633009 Can't boot off XAUI card on Maramba
6631946 (init-program) causes illegal instruction trap if executed when cwp is not 0
6631330 niu driver changes for goa
6629201 maramba post dimm failures must call out the right dimm
6628699 OBP needs to support Maramba platform
6626045 Update Huron RNG OBP virtual-device node
6623916 Software guest state updates generate too much traffic
6623111 Huron system hung after completed POST with "Failed to set device address: 1" with FW 7.0.7
6622775 Running POST with the Neptune FEM installed, disables the PCI-SWITCH
6622444 Boot path switch feature is not work correctly during bootblock load
6621175 False NIU FZC XMAC   Block Port 1 init test failure - RXMAC STATUS Reg. PHY_MDINT Bit
6617193 POST offlines all L2 banks when it encounters a storm of DSC/FBRs
6616363 Glendale's onboard port was not recognized when a Northstar QGC EM card was loaded into the system
6612178 Rev52 Jasper320 cards with v1.13 FCode fails on all Sun platforms
6612022 N1 POST hangs during Enable L2 Cache
6611798 POST support for Turgo
6609130 Monza platform support in OpenBoot
6609024 FERG marks some e-reports from post as invalid and drops them
6608466 GD Post nac names are incorrect
6606197 remove product name from host flash version display
6605782 OBP needs to support the Glendale platform
6604845 Banner does not display the official platform names 
6604051 POST Support for Monza 
6601822 USB hub, keyboard, and/or mouse disappear from OBP device tree
6601551 Use mailbox for systest arguments
6600945 power-off doesn't power off the virtual machine OBP is running within
6598829 ( logo-addr logo-len ) " oem-logo" $setenv is not persistent
6596594 After resetsc, changing OBP nvram parameters do not take affect
6596546 Montoya: "probe-ide" shows a non-existent device with garbage characters as ATAPI model
6595500 Last Trap: Fast Data Access MMU Miss on VDS stress tests
6594929 sun4v systems lost their scsi initiator settings after upgrade to 6.4.x+ firmware
6594395 "Options: true false" menu interrupts OBP reset
6593547 IO-Domain-Reset: ERROR: Last Trap: Watchdog Reset
6593097 POST needs to support SEL_LO_ADR=1 memory addressing
6592986 Add Unix flash update support for U45 MB_PN's 375-3552 and 375-3553 and U25 MB_PN 375-3556
6592973 sata_drive Block error in Hitachi SATA HDDs occurred when power is cycled by s99zzzpc script
6590912 POST needs to clear the FBD syndrome status register twice because of N@ errata #116
6590384 V125(El paso): Could not read diag-level from NVRAM!
6590254 POST is wrongly ASR disabling NIU port in a Single XAUI configuration.
6589571 On OPL XIR at ok? prompt can cause OpenBoot to hang on systems with a large number of strands
6589154 Unexpected traps, L2 UE and lots of error messages in POST when it is faced with FBUs
6588214 Need to remove clock-divisors from v440
6587533 HV Abort: <Unknown?> (82859d0) - PowerDown when starting guest domain that owns bus pci@780
6586400 CR 6554358 breaks builds for excalibur in 4.26.x, 4.25.x,& 4.23.x
6585340 uadmin 2 0 and reboot reads old bootmode settings (should be cleared)
6583392 POST timeouts during PCIE probing (plx errata #7)
6581794 NVRAM configration variable to enable/disable Relaxed Ordering attribute (attr_RO)
6581660 Remove "FBR Error Tally" message in normal verbosity mode
6581490 ERROR: Slave timeout waiting for 6:7 to finish, offlining core 6!
6581085 Can't boot over XAUI network interface
6579294 Enhancements to Systest (test within debug menu)
6576406 POST does not run correctly with disabled L2 cache banks[0-3]
6575253 POST needs to report cpu status by strand
6574105 Issuing a boot to the cdrom device hangs the system if no cdrom media is installed
6574092 change post threshold for fbr screen
6573618 Unused POST code
6573367 Disabling cpu8, disables core1 with failed device:MB/CMP0 (CORE) MAU (ERROR: TEST = MAU GF2M MODEXP) 
6572821 Support FWARC 2007/354.
6570779 post reporting 1/2 of available memory while vbsc and solaris report full amount, 4GB memory only
6570315 Post support for Glendale 
6569526 V445 ships with incorrect devalias paths to interval drives when configured with LSI1068e
6566732 IO operation fails randomly after switch-cpu
6561957 OBP bge ethernet driver needs performnace improvement when load a big file (wanboot 108 MB)
6561842 Putback n2-devel gate into 4.x
6559998 Fix to cr 6520058 can cause FORTH stack corruption. 
6558342 POST ends prematurely after "Copy POST to memory"
6557874 Need clean CP2500 OBP smc kcs interface
6554358 Panther L3Tag failures require a POST base test to be detected 
6553004 Hotplug needs to be enabled on St. Paul
6551724 Booting from DVD on Huron fails.
6550784 Data corruption due to wrong sTLB mapping
6550743 (RFE) Jupiter processor support for OPL platforms
6550717 reset.bin too big. Change the N1 POST PROM offset from 1M to 2M
6550398 flx17584: Observed "/console: error to writing to console"
6550351 Issuing a boot to the cdrom device hangs the system if no cdrom is installed.
6549753 Montoya RTM needs support booting from USB disks.
6548060 Add support in 4.x for N2 based platforms
6547428 the warning message has an incorrect spelling. WARNING: No response from Domain Service "Providor"
6546593 WANboot should not reflect packets
6545566 Sun4v call for dma-sync with zero-length buffer results in hypervisor errors
6545200 OpenBoot should only start CPUs which are part of a domain, as indicated by MD
6545197 OpenBoot should use HV API CPU_YIELD when looping in slave loop
6543749 guest domain : wanboot "miniroot" download takes more than 30 minutes
6543748 gust domain : ERROR: Last Trap Memory Address Not Aligned when "watch-net-all" is interrupted
6543430 OBP should retry a cpu_send_mondo hcall if EWOULDBLOCK is returned
6540632 Need definition of OBP power-off for LDOMs systems
6539675 Fix bugs in Systest (performance counter overflow and malloc_bank for half pop systems)
6538367 Huron ophir eeprom mac address is not getting programmed properly with ILOM
6537035 NIU FCode driver needs to clear remote_fault_detected bit (new for N2 2.0 parts)
6535840 POST needs to implement support for ops-mode
6534031 Stack error in NIU FCode driver
6534028 Unable to boot from NIU port 1 (XAUI0)
6532334 When LDOMs had trouble loading up properly, serial port is unusable
6529934 IO device probing on sun4v platforms needs to be hardware agnostic
6529504 Dropping to ok prompt via send break from running OS causes red state exception
6529467 POST should handle preceeding spaces gracefully
6529207 Compile time complaint in USB2 FCode
6528667 vnet FCode should restrict use of MAC address other then local-mac-address
6528635 Changes to speed up dmake have caused lint_check.pl to misreport
6527778 Net installation of multiple domains results in a hang due to out of order packets.
6526870 OBP should automatically create devaliases based on the devalias properties given by zeus
6526861 St Paul SAS WWID should not be programmed based on system-mac-address at run time.
6526699 Doing a build on all products out of the POST tree is very slow
6526454 St. Paul POST has PCI-EM slots reversed
6526107 St. Paul needs to support booting from USB disks.
6525913 "SUN PROPRIETARY/CONFIDENTIAL" message appears on boot on FCS seattle
6525090 reboot-info can be lost on MD updates
6524613 OpenBoot does not handle LDC resets properly
6523823 St. Paul: EM -> PCI-EM
6523024 the /ebus@800 device nods should not show up in domains that do not also have /pci@780
6521645 vdisk drivers should add a more conservative timeout when waiting for handshake packets
6521605 vbsc times out while waiting for POST progress updates to the sequencer and gets reset
6521198 Incorporate enhanced POST memory tests in POST debug menu
6521186 Incorporate new Systest/Thrasher test in POST debug menu
6520718 OBP should assign MAC addresses to on-board network adapters based on MD info from SP
6520058 Schizo FCode driver does not support CDMA interrupts which can lead to Solaris panic
6519943 after upgrading to fw 6.4.0.build_06, OBP NVRAM parameter "security-mode" gets corrupted
6519920 flx20277: UTP - JLL9.2 OBP firmware breaks Jade/UTP tpdriver attachment, 2 UTP env.
6518883 flx20174: obp command, "test-all", hangs on Jade Jalapeno host & satellite.
6518879 St Paul: POST dimm typo
6518865 St. Paul: PEM -> EM
6518846 St. Paul: PEM -> PCI-EM
6517207 LDOMs OBP commands setenv, set-defaults, set-default to not work
6517108 OBP shouldn't be hard-coding max-#cpus
6516619 OPL showdomainstatus incorrectly reflects real state in XCP 1014
6515491 security-mode has a "Default Value" of "none" instead of "No default".
6513595 OBP needs to support the Sun Blade T6300
6512892 Remove IPMI console abort to workaround 'Memory Address not Aligned' trap on Jade
6512782 Ophir EEPROM reprogramming must be enabled on all platforms
6512314 Jade obp shows 'Don't know the role!' after halt
6512280 Add Device ID for new Shrink DIE of Sansung E$ SRAM to POST device database (POST allows device).
6512278 NIU FCode device driver putback
6511901 Jade console hits 'Memory Address not Aligned' trap
6511659 The eeprom command does not work when running on the factory-default MD set
6510722 errors are not printed out at OBP, when a device or devices are asr disabled
6510693 Joint copyright for Sun/Fujitsu needs to be changed for the year 2007 for OPL OpenBoot binary
6510676 OpenBoot will not build on Solaris 10
6508906 post and obp build issues
6508474 OPL OBP should refer to LSB bitmap instead of HWD data when syncing NVRAM data on all LSBs
6508466 LSBID of new console (upon console switch) needs to be saved in SRAM
6508449 Need to add "domain id" information to OPL OBP error log structure
6508437 A STICK register parity error leaves OPL OBP in hung state
6506771 OBP has platforms which don't build any more because of PROM growth
6505760 when disable first thread of a core, post fails whole core after poweroff/on with FATAL ERROR.
6505657 OPL OBP should restart the domain upon detecting an Oberon PCI Channel marked with a UE
6505653 OPL OBP should reboot domain when encountering the memory UE
6504375 local-mac-address? parameter for OPL OBP should default to true
6504355 Openboot: non-functional sun4v retained-memory code places limitations on mblock size and alignment
6503261 changing NVRAM paramter at OS level causes panic : BAD TRAP: type=31
6500325 OPL OBP should not check Oberon link status if POST has already degraded because of link-up failure
6500287 Release new OBP image for SESI Products with enhanced Panther 2100MHz timing.
6500285 FW keying is required to support UltraIV+ high power modules.
6498780 "Can't locate boot device" message on OPL FF1 and FF2 - IOU slot 0 might be the possible cause
6498373 POST did not run after system firmware was upgraded to SIV 6.4.0_build_02
6495912 VSW: "WARNING: exceeded number of permitted handshake attempts" or loss of network connectivity
6494859 Device alias for "cdrom" is set to wrong path on DC systems
6494774 Add guest-state support for Niagara platforms
6491132 V445 AC power restoring causes OBP post fail
6490115 OpenBoot vdisk driver should be compliant to VIO specification
6488855 flx18074: ERROR: motherboard SEEPROM access failed
6488846 FF2:jasper320 FCode checksum error during POST
6487708 Strengthen request_resource function by adding spin lock around potential race condition
6487438 LDOMs OBP does not correctly handle zero length ldom variable updates
6487348 OBP needs to implement the ASR domain-service outlined in FWARC 2006/594
6487343 OBP's virtual nexus probing code is inconsistent when looking for the "ino" md property
6487332 Unable to update ldom-variables after a halt one a system without domaining enabled
6487301 sun4v OBP does not track physmax correctly in the event of multiple mblocks
6487292 Jade .alarms timer not running after Solaris halt
6487287 The OBP LDC driver should conform to FWARC 2005/571
6487277 ./dimmCheck hangs intermittently when we have 8 x Samsung dimms in a Chicago system
6487271 Legacy nvram svc-channel support should be removed from sun4v OBP
6485941 OBP times out prematurely during vdisk/vnet boot
6485717 LDOMs OBP: "reboot-command" does not work as described in LDOM 1.0 OBP Design Spec v1.1
6484976 Error exception before cpu-struct is initialized can cause the machine to hang-up
6484677 Add support for USB2 under OBP
6482540 Cleanup of POST build targets 
6481980 FCodes for double precision math are broken
6481526 Problem in builiding dropins that share files
6480389 "ERROR: /memory: CPU1 Bank 0 DIMMs are from different vendors"
6480310 Some of the CPU registers printed by OPL OBP do not match SPARC64 extension specification
6478646 PCI bridge probing code does not need to execute config writes to nonexistent devices
6478437 sun4u fire fcode driver initializes 32 bit memory list to incorrect size
6478131 compatible properties for sun4v virtual devices are hard-coded in obp
6474932 Seattle/Boston OBP need to define slot-names property
6474333 POST needs to add support for the LDC console protocol
6472605 Factor niagara-specific code out of sun4v-specific file
6471999 Map-in/out of resources does not works when multiple instances of an Oberon node are opened & closed
6470888 OBP firmware will not update on N210s with 375-3471 mainboard
6470510 Jade does not have transparent PCI-PCI bridge driver. (flx1915)
6470467 Instruction flush and .trap-registers changes
6469964 JLL5.1: POST fails when powering on Jalapeno with high CPU speed 
6468359 POST needs to test all cpus when 'diag-level == min'
6468284 "msi-address-ranges" property for Oberon programmed with wrong values
6467470 Add both Unix and Standalone flash update support for Netra 2x0 R06 Motherboards
6466695 setenv command shows "Usage: setsmcenv option-name valuse
6466679 OPL OpenBoot generates incorrect error log when there is fault accessing Hardware Descriptor table
6466655 OPL Openboot should not do retry when its Oberon leaf link-up attempt fails
6466637 OPL OpenBoot does not accounts for 4k PCIe config space when identifying a faulty device
6466624 OPL OpenBoot generates incorrect error log for faults at PCI-E switch upstream-port on PCI-E IO boat
6466207 Fire PCI-E bridge version should be determined based on fire-revision# rather than module-revision#.
6465254 Change OPL Openboot banner to show "using Domain console" instead of "using Pseudo-SU based console"
6465220 APL/Niagara platforms need multipath boot support
6464267 A single 1050 MHz module produces an error after a soft reset when in diag mode.
6463668 Add Logical Domain Support to OBP source base
6460934 Change messages printed by OPL OpenBoot to protect Sun "OpenBoot" trademark
6460910 OPL OpenBoot should include Fujitsu's copyright in OpenBoot banner
6459574 Need two fail bits to present two additional PCIE-PCIX bridges for          better fault isolation in Pelton.
6459548 If a faulty device cannot be isolated during boot we should try multipath-boot recovery
6459543 Multipath boot should be applied on boot device failure only after image has been loaded from it
6459524 Wrong PCI configuration information being sent to XSCF for PCI-X IOboat on DC model (OPL platform)
6458997 LSI 1064/1068 FCode Port enable command adding too much time to system boot
6457354 d< is broken
6456952 Jade needs to add jalapeno CPU support.
6456885 POST trashes OBP flags
6456539 Release new OBP image for SESI Products with enhanced Panther 2100MHz timing.
6455202 "supported-network-types" on BGE will breaks with 1000Mbps settings
6454051 LSI 1064E compatible property does not match Solaris driver aliases file in s10u2
6452256 OPL OBP to support the new error log format and unit/part codes (name-id) of faulty device
6452237 OPL OBP degrades all SCF paths if it send an SCF command while SCF is busy
6452223 OBP should program "cache-line-size" register for PCIe devices also
6452183 Panther 2100 Ecache timing number change.
6451938 Add POST support for Elpaso
6451762 Add Obp El Paso support
6451721 flash-update command not working for Schumacher
6451168 Fix the 1st level and 2nd level slot-count values for OPL systems
6451159 OPL OBP to ignore bits 0 & 1 of Oberon UBus Device ID reg when creating "module-revision#" property
6451155 OPL OBP need to support IOUs with old (rev 4.3) and new (rev 4.5) NEC PCIE-PCIX bridge
6450624 Disable NPWR_EN on Seattle
6450457 OBP flashupdate from 4.22.11 to 4.22.13 fails with "flash device is write protected"
6449659 Pelton POST PCI id test output incorrect for PCIX and PCIE slots.
6449538 BGE properties hang net boot loading Solaris
6448548 New MB and CP numbers to support Panther 2100.
6448085 post fire2.1 support
6447852 Incorrect value used for stick and tick timer mask
6447824 Cleanup code for error detection/faulty device identification and save-registers-all command
6447821 Chassis serial number should be increased from 8 bytes to 10 bytes on OPL machines
6447820 Stick syncing code in OPL OBP should not use stick counter to check for timeouts
6447818 OPL OBP should not refer to boot-mode flag in HWD to stop auto boot of OS
6447815 SCF selection code would select the last selected SCF even when all the SCF paths have been degraded
6447810 For OPL machine, %tba & %tl should be restored in WDR handler when TBA/TL parity error is detected
6447763 OPL needs Multipath boot support
6447749 OPL OBP needs to create device aliases for 'disk', 'net' and 'cdrom' based on domain configuration
6447642 LSI 1064 fcode modifies latency timer and cacheline size
6447326 Remove CPU speed configuration menu
6447320 Remove OBP flash-update command
6445593 Extra activities on V245's I2C bus may cause false POST failures
6444152 Seattle Unix OBP flash update script needs to support new Seattle MB part numbers
6443014 Sun4v OBP variations should use FWARC approved methods to parse Machine Description data
6442350 U45,fails to negotiate w/the DSS-8+ switch and has no network access when init 6 or reset-all
6441889 OBP needs to support Netra CP3060
6441770 I2C workaround for EPIC access issue
6438710 Platform name for Ontario and Erie has to be changed in POST
6438649 I2C contention between OBP and ALOM
6438159 Seattle OBP needs to support 2UEEL riser card
6436371 OPL OBP need support to degrade a device that executes "abort" while FCode evaluation
6436354 Oberon PCI IO space allocation should start with a non-zero address
6436300 netconsole gets stuck while running obdiag with base fabric interface
6436266 Pseudo-mc node for OPL should not be created for LSBs that have been marked as degraded in HWD
6433152 Add flash update support for RoHS V210/V240 R06 MB_PN's
6432504 Support Jalapeno+ processor on Boston.
6431870 IO forwarding ranges not properly shut down in PCI bridge FCode
6430572 Suppress FCODE map-in whine.
6430500 preprober code touches all devices including devices that are marked bad/blacklisted
6430219 PCI Preallocation code uses 'min' to compare PCI resources which treats value as signed number
6430086 auto-boot? config variable should default to 'true' on OPL machines
6430079 Method pcie-capability-regs in obp/dev/pci/device-props.fth should change as per CR 6420194
6429329 Issuing XIR on OPL machine causes system hang
6428946 Need work around in obp to fix farward reference bug in guest md
6428852 putback for 6395675 panics Boston platform with ereport.io.fire.pec.cto.
6427102 flx18074: ERROR: motherboard SEEPROM access failed
6427093 flx18052: Hot swap may cause chassis-type to be set to zero, FW 4.22.4
6426346	OPL OBP should setup Alive Check execution to detect machine hangs due to transient errors
6425918 POST script needed to track duplicate function declarations
6424812 ereport.io.fire.dmc.tte_inv seen on ontario and ontario+ using system firmware 6.1.9
6424432 Negotiate hypervisor API version 1.0 for the interrupt group id on behalf of legacy Solaris
6423803 OBP support for dynamically programming the SAS WWID
6423795 Serrano support for Schumacher board
6423788 Broadcom 57xx fcode driver support for IPMI/ASF firmware
6423761 wait for doorbell failed,  LSI fcode 1.00.41 needed
6423137 flx18017: netconsole does not get to ok prompt after xir on Jade satellite
6423131	OPL OBP breaks compatibility with PCIe base spec by representing Oberon child devices at device#1
6423090 Fire TLU Ctrl Reg NPWR_EN bit must be set to 0 on Boston.
6423038 Third party graphics card (Barco) not recognized after upgrading OBP 4.9.7 to 4.17.1
6422909 When first power on and at OBP level the wrong characters appear on screen...
6422818 Solaris boot panics on pelton
6422104 Rearrange Oberon driver code to share code between the Oberon leaves
6421977 A WARNING message is seen in POST running with 1GB Infineon DIMM (seattle 1U S163)
6421884 Boston-specific Fire GigaBlaze settings for Optimal PCI-E Signalling
6421866 Boston-specific Fire GigaBlaze settings for Optimal PCI-E Signalling.
6421833 Confusing POST error message "Address does not match in free call" for a CPU failure
6421344 'slot-names' property not created if Oberon leaf link-up fails on OPL machines
6421308 Incorrect "available" property for cmu-ch node in OPL platforms
6420886 POST needs to be enhanced to support Montoya platform
6420241 Make the PLX 8532 PCI-Express workaround for CR 6397497 standard probing procedure
6420194 Need to protect find-std-capability and find-extd-capability from hang due to a bad hardware
6420147 Method 'disable-children' in dev/pci-bridge/dec21152/pcibridg.fth does not disables all children
6420137 Wrong mask used to clear pci errors in  'clear-pci-errs' method defined in obp/dev/pci/pcibus.fth
6420097 phys.hi>cfg-offset method does not work for non-PCIE bridges
6419216 WANBoot : Cannot create ramdisk "ramdisk-bootfs"
6418658 Incorrect paths in seattle ASR
6418642 Net boot failed on Jade platform
6417885 Backout INTX disabling fix (6377849) from OBP
6416671 Jade smc smcenv-sync print wrong data
6416658 POST needs to be enhanced to support Pelton platform.
6416169 flx17820: Dimm1 dimm0 devices disabled Fatal error on Jade
6416142 Disabling components causes MMU miss error in obp probing
6416036 Jade obdiag alarmdiag runs only 3 tests
6415545 FW needs to dump the core shadow scan data on an IERR
6415442 Change Branch Predictor Mode (BPM) in OBP for Panther USIV+.
6414995 Pelton platform support in obp 4.x
6414799 Seattle OBP needs extra guard pages for boot support
6413698 reset-all displays many JBUS-PCI bridge master error logs on a RR chicago system with obp 4.22.5
6413467 Boot from DVD does not works on OPL machines
6412889 Fiesta products with 1MB flash roms do not fit with POST and OBDIAG in the second 512kb
6412550 Montoya needs OBP slot-names property
6412474 OBP find-drop-in? goes out side the flash size and hits the MMU Missing
6412462 Jade sat's mcnet does not work properly on 4.22.4 OBP.
6411912 POST fails scrub memory
6411069 OBP PLL data writes should be consistent with POST.
6411051 ASR disabling PCI slots does not always work.
6409416 Add watchdog timer support to OBP
6407889 Add 2UXXL support, remove 2UEXL support
6407069 flx17690: ERROR: no valid memory configuration, System config failed,powering off on Jade
6406577 Hotplug Allocation Support needed in OpenBoot
6406195 "Change Southside obp's root name"
6406142 PCI bridge code handles IO limit = 0 incorrectly
6406091 Fix some stack comments and nits in common OBP code
6406061 Fix the decoding of 'movr' instructions in OBP sources
6404798 Host keeps on resetting when keyswitch is set to diag.
6403073 Serranos with no memory may report false POST errors - CTRL/C; POST error & poweroff(P1.0 S#133)
6402909 PoST change required to implement Spread Spectrum J-Bus Clock
6402905 OBP change required to implement Spread Spectrum J-Bus Clock.
6401719 IO-Bridge Error - Data miss compare when running DMA loopback mode. 
6401634 Olympus Product Line (OPL) system support in OBP 4.x gate
6400408 Modify RX_EQLIZR_CTL bits in Seattle Fire LPU Gigablaze Glue Config2 Register to 0000 from default
6400192 Boston OBP needs extra guard pages for boot support.
6400117 cdrw -p24 command does not work correctly on T2000.
6399627 Southside suport in post 
6399215 Add Southside support
6397564 calls to hypervisor version API need to be specific to a cpu architecture
6397497 Boston (V445) will not boot with LSI20320-S (Meteor) HBA installed.
6397170 missing device_type property on ebus bus node properties
6396546 Remove pre-P1.0 hacks
6396540 Program static SAS WWID at boot time
6396533 Solaris flash-updater broken
6396528 PCI-X out of band riser card interrupts should only be created if 2UEXL or 2UEEL riser card used
6396519 OBDiag EPIC test fails
6396464 interrupt-cells property in the ebus node has a typo in it.
6396318 Printed date in OBP is off-by-one after 28-feb 2006.
6395015 2Gigabit/Sec Single FC Host Adapter (JNI) Last Trap: Data Access Error.
6394040 OBP doesn't handle low-cost keyboards without bCountryCode byte
6393958 Jade (CP2500) needs to add hybricon chassis support.
6393953 Updated P5 firmware/obp an entra "cr" in console-filter of ipmi-serial.fth
6393665 Solaris flash-update script fails.
6393492 Need to enforce memory CAS latency minimum of 2.5 on DIMMS running at more than 133MHz
6392873 reset-all after asr-clear executed makes OBP ERROR: motherboard SEEPROM access failed.
6392749 Add support for decoding Serrano specific AFSR register bits
6392744 Netra 240 OBP should support Serrano and Jalapeno CPUs dynamically
6392742 Netra 440 OBP should support Serrano and Jalapeno CPUs dynamically
6392539 Volume type is being referenced instead of volume id in 1.00.39 1064 fcode
6391455 * Create reg property directly rather than with ebus code
6391361 post and picl DIMM labels are different.
6390564 Pelton does not provide slot-names property
6390526 USB 2.0 Hub gets lost to OBP after Solaris EHCI driver run
6389988 POST Prints out DIMM #'s instead of proper nomenclature
6389161 Fire rxeq values not optimized for ontario
6388925 Alom Obdiag subtests are not available in test option menu.
6388673 POST fails IO-Bridge unit 1 at address 00000400.0f701400
6388582 add hypervisor/supervisor split for n2
6388093 Wanboot with S10_U1 miniroot panics with "map_prom: prom i/o page without side-effect"
6387399 VPCI fcode: Access to PCIE extended config space does not work correctly
6386341 post needs to check link width for onboard devices
6386216 Changes to MD's in vBSC need to be reflected in OBP
6385582 VBSC and POST have different memory size
6384845 local-mac-address support does not works on OPL machines.
6384335 chicago unable to boot off network port 1
6383658 Dynamic FRUID writes cause OBP MB FRUPROM reads to fail
6383237 nvramrc must be evaluated before probe-all
6382974 Schumacher IPMC device node creation faults.
6381818 stand-init debug functionality does not work as expected
6381385 Upgrade LSI 1064 FCode to 1.00.39
6381283 sun4v platform support
6381281 bge fcode should support device args and properties specified in FWARC/2002/345
6381279 Remove no-probe-list property from Fire nodes
6381277 Interpreter workarounds for historical/legacy fcode prom bugs must be removed
6381274 Code restructuring changes needed for proper vfcode tracking
6381272 Use system-tick-speed instead of ms-factor to measure time
6381271 All configuration variables should be set to defaults on NVRAM initialization
6381242 Seattle platform support
6381125 ERROR: The following devices are disabled: ide.
6381115 mixed speed memory will not interleave in enchilada system
6381105 obp needs to support RoHs scsi disk bkpln 501-7344 for Netra 440
6381084 bootmode reset-rvram does not reset nvram variables.
6381064 System cannot boot with input set to type-7 keyboard plugged into front Ontario T2000 usb port.
6380975 "Chicago/Southside does not provide slot-names property"
6380622 menus in post shows incorrect number of CPUs
6380442 Seatle_P0.1-2U: FATAL: no exception frames available, forcing misaligned trap (S#S020)
6379979 fcode: map-in of config space does not work correctly
6379878 Chicago OBP should tune ebus chip select timing as an intermediate step towards meeting STARS 
6379876 USB time out errors seen in OBP during power-cycle testing 
6379703 POST for St Paul
6377849 Need to disable INTX prior to boot
6377208 Jade B8.1 : boot F/W debug messages has been seen druing reboot after updating SMC firmware
6377038 Jade B8.1: In cPSB, "Warning: Fcode sequence resulted in a net stack depth change of -3" in reset
6376657 OBP I2C Drivers should frame each unique addressed device with a START and STOP.
6376524 show-sensors output values are incorrect.
6375990 Make all I2C transactions including errors send a stop
6375003 nvram access faults when dropping from Solaris to OBP.
6374738 Address for PSU0's fruid prom needs to be 0x24 for P1.0 Boston.
6372564 Preparing for new niagara platforms
6372458	Boston PCIX interrupt maps incorrect.
6370408 flx17072: Jade satellite goes to 'config" when powering off while rebooting. B8.
6370405	flx17062: Jade satellite on B8 does not use the FRU Boot_Devices correctly.
6370015 OBP should print out a message if it detects problem and resets RTC
6368716 bringover -g; make from OBP 4.x gate fails for boston
6368614 WARNING: devinfo: fault in private data at 60000d794e8
6366588 fcode gives erroneuos values for config address > 0xf.0000
6364139 OBP shows "ERROR - BCM5714 device 0 missing" with pci1 is disabled.
6361563 POST failed: 0>ERROR: TEST = IO-Bridge unit 1 int init test
6361535 POST needs to be enhanced to support Netra(tm) CP2500
6361002 Jade B7: obdiag hangs at serial console test
6360432 Porting 4.x OBP to Jade (Netra CP2500) platform.
6347549 Request to have test name convention to identify between Test, subtest, message, etc. 
6347502 Request for adding timestamps to POST code
6347315 unused POST modules/routines
6346885 OpenBoot does not handle Non-Resumable Error traps
6346530 sun4v OBP needs to support versioning APIs
6345852 flx16583: On Jade system the uname -i is reporting the wrong thing.
6338777 Prevent ufsboot giving divide-by-zero from bad argument
6333076 ontario 1064 onboard support
6332576 updates to pciid test for unknown devices
6322957 wrong POST and OBDiag version printed out at ok prompt
6313800 OBP should read and print the 'test release' flag while printing H8 firmware version
6256046 RFE: help for "post" should bring up help for diag
6244643 Need to modify initialization time of 2X Slimline DVD-R/-RW drive to much lesser time
6230541 ERROR: Timeout on 0 waiting for resource type 2. after a ctrl-c when memory is being initialized
6230349 Fix spelling in .controls word in obdiag/lib/error.fth
6183557 forth.exe uses tokenize.exe which violates the SPARC ABI causing a SEGV crash
6181985 local-mac-address of bge interface is seen on pci card when net  NVALIAS is duplicated
5079227 This, ")" in between "Copyright" and "2004", is not in the right place.
5079065 Make OBP support mapping devices into 64 bit address space on PCI-E bus
5076888 asr disabling all memory banks and a reset causes the system to shutdown.
5052695 post off doesn't run at diag-level off
4946025 WARNING: ce0:interrupt #0 has been blocked
4854322 The idprom node is missing its close method.
4794955 POST debug menu's help not implemented

Patch Installation Instructions:
===============================
Please refer to the Install.info file for instructions on updating the
firmware using the files included in this patch.  
 
Note:
=====
After the release of the first version of this patch (-01), a regression
was discovered that affects only certain configurations of the UltraSPARC
IIIi platforms using the first generation of PCI bus interface controller,
including the platform utilizing this patch release.  The problem may cause
a system to fail to boot if it has certain PCI cards installed in affected
PCI slots.  If this problem occurs, the system will display the following
error message on boot:
 
     ERROR: <pci_device_path>/<Unnamed>: Last Trap: Data Access Error
 
This is a known issue (CR 6890136) and is to be fixed in OBP 4.30.4.a.  For
systems that experience this issue, there are two workarounds.  Either move
the affected PCI card to a different slot, or downgrade your firmware to
the prior release until the -02 version of this patch is available.  Full
details on this issue are documented in CR 6890136.
 
*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-

Special Install Instructions:
0

README -- Last modified date:  Thursday, February 11, 2010

