| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
OpenVMS VAXSYSL02_2H455 VAX V5.5-2H4 SYSLOA/Error Formatter ECO Summary
    TITLE: OpenVMS VAXSYSL02_2H455 VAX V5.5-2H4 SYSLOA/Error Formatter ECO Summary

    Modification Date:  29-JUL-98
    Modification Type:  New Kit

    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1998.  All rights reserved.

    OP/SYS:     OpenVMS VAX

    COMPONENT:  Error Formatter
                SYSLOA

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXSYSL02_2H455
         ECO Kits Superseded by This ECO Kit:  VAXSYSL18_U2055 (For OpenVMS
                                                 V5.5-2H4 *ONLY*)
         ECO Kit Approximate Size:  2142 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2H4
         System/Cluster Reboot Necessary:  Yes
         Rolling Re-boot Supported:  Yes
         Installation Rating:  3 - To be installed on all systems running
                                   the listed versions of OpenVMS which
                                   are experiencing the problems described.}

         Kit Dependencies:

           The following remedial kit(s) must be installed BEFORE
           installation of this kit:

             None

           In order to receive all the corrections listed in this
           kit, the following remedial kits should also be installed:

             None

    ECO KIT SUMMARY:

    An ECO kit exists for SYSLOA and the Error Formatter on OpenVMS VAX
    V5.5-2H4.  This kit addresses the following problems:

    Problems addressed in VAXSYSL02_2H455:

      o  The VAXSYSL18_U2055 multi-version kit is being re-issued as
         separate kits.  If you have installed the VAXSYSL18_U2055
         remedial kit you do not need to install this kit.

    Problems addressed in VAXSYSL18_U2055 for OpenVMS VAX V5.5-2H4:

      o  Previous SYSLOA kits have been combined into one kit.  All
         the problem solutions that were in the kits superseded by
         VAXSYSL18_U2055 are included in VAXSYSL18_U2055 and apply
         to versions 5.5-2 and 5.5-2H4 of OpenVMS VAX.

         NOTE:  The following SYSLOA*.EXEs are included in this
                ECO kit and are used with the CPU types shown:

                SYSLOA1202     VAX 6000-500
                SYSLOA1302     VAX 6000-600
                SYSLOA1303     VAX 4000-100/100A/105A   MicroVAX 3100-90/95
                SYSLOA1701     VAX 7000/10000
                SYSLOA420                               MicroVAX 3100
                SYSLOA440      VAXstation 4000-VLC      MicroVAX 3100-30/40
                SYSLOA46       VAXstation 4000-60       MicroVAX 3100-80
                SYSLOA49       VAXstation 4000-90
                SYSLOA43       VAXstation 3100 M76
                SYSLOA43D      VAXstation 3100 M76/GPX
                SYSLOA43S      VAXstation 3100 M76/SPX
                SYSLOA43W      VAXstation 3100 M76 (MONOCHROME)
                SYSLOA9CC      VAX 6000-200/300
                SYSLOA9RR      VAX 6000-400

         ***********************  WARNING  ****************************
         *                                                            *
         *  If you are going to install this ECO kit on a VAXstation  *
         *  4000 Model 60 or VAXstation 4000 Model 90 system that has *
         *  a TURBOchannel device installed *AND* is a member of a    *
         *  VAXcluster, you *MUST* install CSCPAT_1045 on your        *
         *  system either before or in the same installation session  *
         *  with this ECO.  If this ECO is installed on a             *
         *  system that meets the requirements mentioned above,       *
         *  the system will crash at boot time with an INVEXCEPTN     *
         *  bugcheck at STACONFIG+578A if CSCPAT_1045 does not        *
         *  exist on the system.                                      *
         *                                                            *
         *  If you install both kits during the same session,         *
         *  Digital recommends that you do not reboot between the     *
         *  application of the two ECO kits due to the probability    *
         *  of a system bugcheck which causes an unbootable system    *
         *  if only this ECO is installed.                            *
         *                                                            *
         *  For more information, please see the following article:   *
         *                                                            *
         *      *OpenVMS] CSCPAT_1045 SYSGEN, STACONFIG And           *
         *                TURBOchannel ECO Summary                    *
         *                                                            *
         **************************************************************

      o  ANALYZE/ERROR returns an ACCVIO while processing a memory error
         packet.

      o  The VAXstation Model 90 hangs when the VME B board is accessed
         after reset.

      o  ANALYZE/ERROR report does not call the VAXstation 4000-VLC and
         MicroVAX 3100-30, -40 a KA45 as it should.

    INSTALLATION NOTES:

    The images in this kit will not take effect until the system is
    rebooted.  If there are other nodes in the VMScluster, they must
    also be rebooted in order to make use of the new image(s).

    If it is not possible or convenient to reboot the entire cluster at
    this time, a rolling re-boot may be performed.
Files on this server are as follows:
    »vaxsysl02_2h455.README
    »vaxsysl02_2h455.CHKSUM
    »vaxsysl02_2h455.CVRLET_TXT
    »vaxsysl02_2h455.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company