| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxmscp09_u2055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1996.  All rights reserved.

    PRODUCT:    OpenVMS VAX

    COMPONENT:  MSCP (Mass Storage Control Protocol)

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXMSCP09_U2055
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  95 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4, V5.5-2HF
         System/Cluster Reboot Necessary:  Yes

         NOTE:  In order to receive the full fixes listed in this kit,
                the following remedial kits also need to be installed:

                     VAXSHAD09_U2055

    ECO KIT SUMMARY:

    An ECO kit exists for MSCP on OpenVMS VAX V5.5-2 through V5.5-2HF.  This
    kit addresses the following problems:

      o  In the VAXSHAD09 remedial kits, there were four extra fields added
         to the end of the IRP (I/O Request Packet) data structure.  These
         extra fields are past the end of the IRP size so are not zeroed at
         the time the IRP is allocated.  This can result in members being
         thrown out of the shadowset and/or errorlog entries.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system must
    be rebooted.  If the system is a member of a VMScluster, the entire
    cluster should be rebooted.
Files on this server are as follows:
    »vaxmscp09_u2055.README
    »vaxmscp09_u2055.CHKSUM
    »vaxmscp09_u2055.CVRLET_TXT
    »vaxmscp09_u2055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company