| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxcliu02_u2055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1994. All rights reserved.

    OP/SYS:      OpenVMS VAX

    COMPONENTS:  DYNSWITCH.EXE

    SOURCE:      Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXCLIU02_U2055
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  75 blocks
         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4
         System Reboot Necessary:  Yes

    ECO KIT SUMMARY:

    An ECO kit exists for DYNSWITCH.EXE on OpenVMS VAX V5.5-2 through
    V5.5-2H4.  This kit addresses the following problems:

    Problems addressed in the VAXCLIU02_U2055 kit:

      o  When attempting to setup dynamic asynchronous DECNET, if noise
         appears on the line before the DDCMP protocol has been
         successfully established, an infinite loop can be entered.  The
         process ties up 100% of the CPU resources and will remain in
         this state until it is manually stopped.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system
    must be rebooted.  If the system is a member of a VAXcluster,
    the entire cluster should be rebooted.
Files on this server are as follows:
    »vaxcliu02_u2055.README
    »vaxcliu02_u2055.CHKSUM
    »vaxcliu02_u2055.CVRLET_TXT
    »vaxcliu02_u2055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company