| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxmont04_u2055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1996.  All rights reserved.

    PRODUCT:    OpenVMS VAX

    COMPONENTS:  MONITOR.EXE
                 SPISHR.EXE
                 VPM.EXE

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXMONT04_U2055
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  420 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4, V5.5-2HF
         System/Cluster Reboot Necessary:  Yes

         NOTE:  In order for the images in this remedial kit to execute
                properly, the VAXSHAD09_U2055 remedial kit for OpenVMS VAX
                V5.5-2 must be installed first.  If you have not yet
                installed this kit, for assistance in obtaining the
                VAXSHAD09_U2055 remedial kit please contact your normal
                Digital support channel.

    ECO KIT SUMMARY:

    An ECO kit exists for MONITOR, SPISHR, and VPM on OpenVMS VAX V5.5-2,
    V5.5-2H4, and V5.5-2HF.  This kit addresses the following problems:

      o  When the MONITOR command is issued as follows:

              MONITOR IO, PAGE

         or with any other class list, the MONITOR command will fail with a
         remote node exit failure.

         This problem is corrected in OpenVMS VAX V6.1.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system must
    be rebooted.  If the system is a member of a VAXcluster, the entire
    cluster should be rebooted.

    NOTE:  In order for the images in this remedial kit to execute properly,
           the VAXSHAD09_U2055 remedial kit for OpenVMS VAX V5.5-2 must be
           installed first.  If you have not yet installed this kit, for
           assistance in obtaining the VAXSHAD09_U2055 remedial kit please
           contact your normal Digital support channel.
Files on this server are as follows:
    »vaxmont04_u2055.README
    »vaxmont04_u2055.CHKSUM
    »vaxmont04_u2055.CVRLET_TXT
    »vaxmont04_u2055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company