| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxlmf01_u2055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1996.  All rights reserved.

    PRODUCT:    OpenVMS VAX

    COMPONENT:  License Management Facility (LMF) - LMF$LURT.DAT

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXLMF01_U2055
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  100 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4
         System/Cluster Reboot Necessary:  No

    ECO KIT SUMMARY:

    An ECO kit exists for LMF$LURT.DAT on OpenVMS VAX V5.5-2 through
    V5.5-2H4.  This kit addresses the following problems:

    Problems Addressed in the VAXLMF01_U2055 Kit:

      o  The VAX 7000/10000 Model 800 CPUs have different LURT unit
         requirements than the Model 600 CPUs.  With the COMPAT_MODE set to
         V55, the Model 800 CPU is presented to OpenVMS VAX 5.5-2 as a Model
         600 CPU.  Therefore, the LURT UNIT requirements must be modified to
         operate the Model 800 CPUs.  This kit provides the correct LURT
         units to allow recognition of the Model 800 as a valid system.

         It should be noted that this fix has the following restrictions:

           -  Support for the Model 700 on OpenVMS VAX V5.5-2 is not
              provided.

           -  More than 4 Model 600 processors on OpenVMS VAX V5.5-2 is not
              supported.

           -  The maximum memory supported on Model 800 with OpenVMS VAX
              V5.5-2 is restricted to 512MB.

           -  Model 600 systems are *not* supported on V5.5-2 with the LURT
              this kit applied.

    INSTALLATION NOTES:

    The system does not need to be rebooted after this kit is installed.
    However, if you have other nodes in your OpenVMS VMScluster, they should
    be rebooted or you should install this kit on each system in order to
    make use of the new image(s).
Files on this server are as follows:
    »vaxlmf01_u2055.README
    »vaxlmf01_u2055.CHKSUM
    »vaxlmf01_u2055.CVRLET_TXT
    »vaxlmf01_u2055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company