| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxlavc01_2h4055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1996.  All rights reserved.

    PRODUCT:    OpenVMS VAX

    COMPONENT:  PEDRIVER

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXLAVC01_2H4055
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  198 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2H4
         System/Cluster Reboot Necessary:  Yes

    ECO KIT SUMMARY:

    An ECO kit exists for PEDRIVER on OpenVMS V5.5-2H4.  This kit addresses
    the following problem:

      o  Nodes in an LAVC may generate CLUEXIT bugchecks in a mixed
         Enet/FDDI environment where duplicate hello messages are being
         produced (i.e., where the bridge firmware is out-of-rev).

         This problem is corrected in OpenVMS VAX V7.0.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system
    must be rebooted.  If the system is a member of a VAXcluster, the
    entire cluster should be rebooted.
Files on this server are as follows:
    »vaxlavc01_2h4055.README
    »vaxlavc01_2h4055.CHKSUM
    »vaxlavc01_2h4055.CVRLET_TXT
    »vaxlavc01_2h4055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company