| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vax_tw_y2k01_062

    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1998.  All rights reserved.

    Modification Date:  12-JUN-98
    Modification Type:  New Kit

    OP/SYS:     OpenVMS/Hanyu VAX

    COMPONENT:  Year 2000 Fixes

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAX_TW_Y2K01_062
         ECO Kits Superseded by This ECO Kit:  None
         ECO Kit Approximate Size:  388 Blocks
                        Saveset A - 126 Blocks
                        Saveset B - 126 Blocks
                     Cover_Letter -  10 Blocks

         Kit Applies To:  OpenVMS/Hanyu VAX V5.5-2, V5.5-2H4, V6.2
         System/Cluster Reboot Necessary:  No
         Rolling Re-boot Supported:  Not Applicable
         Installation Rating:  1 - To be installed on all systems running
                                   the listed version(s) of OpenVMS.
         Kit Dependencies:

           The following remedial kit(s) must be installed BEFORE
           installation of this kit:

             VAXY2K0n_U2055 for V5.5-2 and V5.5-2H4
             VAXY2K0n_062 for V6.2

           In order to receive all the corrections listed in this
           kit, the following remedial kits should also be installed:

             None.

    ECO KIT SUMMARY:

    An ECO kit exists for OpenVMS/Hangul VAX V5.5-2 through V6.2.  This kit
    addresses the following problems:

      o  The OpenVMS/Hanyu HDUMP utility, which supports the ODS-1
         file system using a 2-digit year format, has been modified to
         correctly interpret these 2-digit years until the year 2057.

         There is more information regarding OpenVMS Fixes for the
         Year 2000 issues at the following URL on the world-wide web:

           http://www.openvms.digital.com/openvms/products/year-2000

    INSTALLATION NOTES:

    Files on this server are as follows:
Files on this server are as follows:
    »vax_tw_y2k01_062.README
    »vax_tw_y2k01_062.CHKSUM
    »vax_tw_y2k01_062.CVRLET_TXT
    »vax_tw_y2k01_062.a-dcx_vaxexe
    »vax_tw_y2k01_062.b-dcx_vaxexe
    »vax_tw_y2k01_062.c-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company