  The terse LAT connection question dept 
 The Question is:
 
What command do I use to connect my VMS system to a terminal server using LAT?
 
 The Answer is:
 
  Your question is sufficiently terse as to be difficult to answer.
 
  The usual command used for connecting from OpenVMS to a DECserver
  terminal server for server management purposes depends on the local
  MOP configuration, with LANCP and DECnet Phase IV NCP CONNECT being
  among the more common approaches used for MOP-based management.
 
  If the DECserver is offering inbound services such as a remote modem
  for dial-out, you can use the DCL command SET HOST/LAT, assuming that
  out-bound LAT has been configured on the OpenVMS System and the
  terminal server is set for inbound (remote, incoming) connections.
 
  There are other potential approaches, depending on the particular
  environment -- please contact the Compaq Customer Support Center for
  assistance.
 
