  Multiple Ethernet Controllers? 
 The Question is:
 
Can I use two ethernetdrivers (two segments) with VMS7.1 and UCX4.2 on the
 platforms AlphaServer800 and DS10.
 
If so, any limitations.
 
If not, what is required for these platforms.
 
Rgds,
Magnus
 
 The Answer is:
 
  Multiple Ethernet Controllers are supported by OpenVMS.
 
  TCP/IP Services V5.0A or later (with current ECO) is strongly
  recommended on V7.1 and later.
 
  For IP, the use of multiple subnets is recommended.
