  OS/2 NDIS and DE210 Ethernet configuration? 
 The Question is:
 
There was a response to someone's question about a
Digital DE210 MCA Ethernet adapter which was very
helpful and pointed me to the drivers for the card.
Unfortunately my system hangs on boot up when the driver
is loaded. I noticed that memory addressed being used by
the driver does not correspond to the address allocated
by the PS/2 BIOS. The PS/2 BIOS setting was C8000-CFFFF,
but the driver displayed MEM 0800-0FFF. The I/O  address
and IRQ were the same as the BIOS setting though.
 
I am attempting to use the driver with IBM's TCP/IP for OS/2,
and there is an NDIS driver available for OS/2 in the E2KIT201.ZIP
file which I downloaded from Digital's Web site, so I would expect
it to work.
 
Any help would be appreciated.
 
 The Answer is:
    You have reached the OpenVMS Wizard. It sounds like you need the OS/2
    Wizard.
