  Typical DECserver 90M Boostrap Time? 
 The Question is:
 
How long should it take for a Decserver 90M to boot?
We just got our first 90M, and it takes about 6 minutes
to come up.   If I monitor the 90M from port 1 i see the
messages that it is loading from flash, and within a few
seconds it displays Image load complete.  The problem is
now it takes about 5 minutes before it says Software
Initialization complete.  In between the messages "Image
load complete" and "Software initialization complete" the
port LEDs cycle between (1-4 on, 5-6 off) and (1-4 off,
5-6 on).  Is this normal, or is it doing something screwy?
 
 
 
 The Answer is:
 
  Recent versions of the DECserver 90M program image have exceeded the
  capacity of the flash RAM, and are thus compressed -- decompression
  times  circa 5 minutes or more (depending on version) are not unusual.
 
