Introduction
Step 1:
Connecting Local Cables
Step 2:
Connecting the Modem
Step 3:
Connecting Power
Step 4:
Start Your Computer
Step 5:
Recording Internet Settings
Step 6:
Reconfigure Your PC
Step 7:
Installing Software
Troubleshooting
Troubleshooting DI-701 Quick Starter Guide Cabling The most common problem associated with Ethernet is bad cabling. Make sure that all conected devices are turned on. On the top of the of the DI-701 is a bank of LEDs, as a first check verify that the Local Link and Internet Link LEDs are lit and green. If they are not, verify that you are using the proper cables. From the DI-701 directly to a PC, the cable should be an Ethernet cross-over cable. From the DI-701 to a hub or switch, the cable should be a straighthrough to a normal hub/switch port, or a cross-over to an uplink port. For the DI-701 to a cable/DSL modem, it is most common to use a cross-over, and it is recommended that you use the same cable as supplied by your modem maker. I can't Find the DI-701 using the DI-701 Setup Software For the DI-701 Setup Software to find the DI-701, it has to be accessed from a client. This means that the computer you are trying to use to run the software must be setup as in Step 6. Additionally the computer should have been restarted to ensure that it is receiving its IP address from the DI-701. To verify that your computer is setup properly use the "winipcfg" utility in Windows. To run this go to Start-->Run... and type "winipcfg" in the Run box. Press the "More Info" button on the bottom right and make sure your network adapter that is attached to the DI-701 is selected in the Ethernet Adapter Information box. Look at the box labeled DHCP Server, this should be the DI-701's IP address (192.168.0.1 as default). If it is not, or it is blank or reads 255.255.255.255 then you may have a cabling problem (see above), or you may have another DHCP server on your network. In either case, please follow the installation guide again, and ONLY connect the client, DI-701 and your modem. If you are on a network, it is recommended that you contact your IS manager for further assistance with DHCP settings. My Internet application won't work To protect your computer from Hackers, the DI-701 uses port blocking. A port is like a door into your computer. Each service on the Internet has an associated port. The DI-701 protects your computer by closing certain ports off so that malicious programs can't access your computer. Sometimes, however, you are using an application on purpose that uses one of these blocked ports. In this case you will have to manually open the port to allow the application to work properly. Some applications that may be affected: Some Email Programs Some Multi-Player Games Some Internet Phone/Video Conferencing Applications The first thing you will need to do is determine what port or ports the application uses. Typically the fastest way to find this information is to go to the software maker's web site. Go to their support section and look for information related to NAT, Proxy Server, or Firewall. This information will typically list 1 to 3 ports that need to be opened for proper operation of the software. If you can't find the necessary information, call the software maker and ask what ports need to be opened for the software to work through a firewall. Once you have the necessary port information, it is a simple matter to actually open the ports on the DI-701. A. Launch the DI-701 Setup Software and press "Find". Once the DI-701 Setup Software finds the DI-701, press "Configure": B. Choose the "Virtual Server" tab: C. Enter one of the port numbers that your application requries and then press the "Browse" button: D. Choose the computer that is using the application and press "Select": E. Press Add. Repeat this process for each individual port you need to open. F. Press Save. Your application should now work. It may be necessary to restart your application or your computer for the application to recognize the change. Getting Technical Support D-Link provides free technical support. North American customers can contact D-Link technical support through our web site, e-mail, or by phone. North American technical support is available Monday through Friday from 6:00 a.m. to 6:00 p.m. (PST).
Web: | http://www.dlink.com
E-mail: | tech@dlink.com
Phone: | 949-788-0805 (option #4)

© 1999 D-Link Systems, Inc. All rights reserved.