**
**
**  D-Link DFE-530TX+ PCI Fast Ethernet Adapter (rev F)
**
**  NDIS Driver for Windows 95OSR2/98/98SE/ME/2000/XP/SRV2003
**
**  v3.46   May, 2005
**
**

Introduction:
=============

  This document shows you how to setup the driver in Windows operating system.

Contents of the Subdirectory:
=============================

    DLKFET5A.SYS        The NDIS5 driver for Windows 98/98SE/ME.
    DLKFET5B.SYS        The NDIS5 driver for Windows 2000/XP/SRV2003.
    DLKFET4.SYS         The NDIS4 driver for Windows 95OSR2.
    NETDLFET.INF        The installation information file.
    WINNDI.DLL          The Co-installer for Windows.
    VUINS16.DLL         The Un-installer for Windows.
    VUINS32.DLL         The Un-installer for Windows 2K/XP/SRV2003.
    WIN.TXT             This file.

Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Turn on the power of your PC on to boot from Windows operating system.
       Windows will auto-detect your new adapter, and the "New Hardware Found"
       dialogue box will appear. Select "Driver from disk provided by hardware
       manufacturer" to install driver from the diskette that comes with your
       LAN adapter.

    2. Insert this CD into your CD ROM drive, and specify the path of the driver 
       in the CD (D:\setup\Windows, assume D: is CD drive),  to copy the driver files to your 
       system.

    3. When the driver installation is completed, restart Windows.


  Note:

    1. In Setup Option "Flow Control":
       When setting to Hardware Default(Auto), the flow control setting is 
       according to the auto-negotiation result based on PHY hardware default
       values. However, when setting to other values(Disable, Enable), driver 
       will just disable or enable flow control ability according to your setting.


