Windows 95

Installation:
-------------
Follow the steps to install the D-Link DFE-690TXD CardBus PC Card's 
driver:

    1. Start your PC, then insert the D-Link DFE-690TXD CardBus PC Card
       into an available PC Card slot in your PC .

    2. After starting Windows 95, the D-Link DFE-690TXD CardBus PC Card 
       will be detected automatically, then the Update Device Driver 
       Wizard window appears.

    3. Insert the D-Link DFE-690TXD CardBus PC Card Installation disk
       into CDROM disk drive.

    4. Click the Next button in the Update Device Driver Wizard window.
       Win95 will start to search CDROM drive for network driver,
       and Windows displays the message

            "D-Link DFE-690TXD CardBus PC Card"

    5. Click the "Other Location..." in the Update Device Driver Wizard
       window, then the Select Other Location window appears.

    6. Type type the path that matches the CD-ROM drive on your system.
       For example, enter the following path: E:\W95_OSR2 and click OK 
       button to install D-Link DFE-690TXD CardBus PC Card driver.

    7. Click Finish button,
       then the Win95 starts to copy the D-Link DFE-690TXD CardBus PC Card
       driver to the user's hard disk.

    8. If Win95 prompt you :
       "The file 'DLKRCB.SYS' on D-Link DFE-690TXD CardBus PC Card
       Driver Disk could not be found",
       "Insert D-Link DFE-690TXD CardBus PC Card Driver Disk into the
       drive selected below and, click ok", fill the "Copy file from:"
       Type the path that matches the CD-ROM drive on your system.
       For example, enter the following path: E:\W95_OSR2

       Then click ok.

    9. Restart your computer.
